## JA8.5 Marking

Light sources meeting the requirements of this Appendix shall be marked with “JA8-2016” to indicate their compliance with the criteria of this Appendix. Light sources that have passed the Elevated Temperature Life Test shall instead be marked with “JA8-2016-E”, to indicate that they comply with this Appendix and may additionally be installed in elevated temperature applications such as enclosed fixtures. Light sources that do not comply with this Appendix shall not be marked with “JA8-2016” or “JA8-2016-E”.