###### Section 140.4(h)2 – Link to Tables 110.2-A-Table 110.2-I

'Standards

Table 110.2-A ELECTRICALLY OPERATED UNITARY AIR CONDITIONERS AND CONDENSING UNITS – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-B UNITARY AND APPLIED HEAT PUMPS, MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-C AIR-COOLED GAS-ENGINE HEAT PUMPS

Table 110.2-D WATER CHILLING PACKAGES – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-E PACKAGED TERMINAL AIR CONDITIONERS AND PACKAGED TERMINAL HEAT PUMPS – MINIMUM EFFICIENCY REQUIREMENTS

Table 110.2-F HEAT TRANSFER EQUIPMENT

Table 110.2-G PERFORMANCE REQUIREMENTS FOR HEAT REJECTION EQUIPMENT

Table 110.2-H Electrically Operated Variable Refrigerant Flow (VRF) Air Conditioners
Minimum Efficiency Requirements

Table 110.2-I Electrically Operated Variable Refrigerant Flow Air-to-Air and Applied Heat Pumps - Minimum Efficiency Requirements