## JA8.3 Tests to be performed

Compliance with the requirements of this Appendix shall be determined by performance of the following test procedures, as applicable to the type of light source.

Sample size for lamps with ANSI standard bases and that are not recessed downlight retrofits, shall be 10 units per model: 5 units tested base-up and 5 units tested base-down unless the manufacturer restricts specific use or position. If position is restricted, all units shall be tested in restricted position. Test units, including low voltage lamps, shall be operated at rated voltage.

Sample size for all other sources shall be 3 units, tested in accordance with manufacturer’s installation instructions for intended orientation.

### JA8.3.1 Efficacy Test

Efficacy at full light output shall be determined by the following test procedures, as applicable to the type of light source:

a) For incandescent and incandescent reflector lamps: 10CFR 430.23(r).

b) For medium base compact fluorescent lamps: 10CFR 430.23(w).

c) For general service fluorescent lamps: 10CFR 430.23(r).

d) For fluorescent lamps that are not Medium base compact fluorescent lamps and general service fluorescent lamps: IES LM-9.

e) For LED light sources, IES LM-79.

f) For high intensity discharge lamps, IES LM-51.

g) For induction lamps, IES LM-66.

(i)

The reported value shall be the minimum efficacy of the tested units and be rounded to the nearest tenth.

### JA8.3.2 Power Factor Test

Power factor shall be measured at full light output in accordance with ANSI C82.77, Section 6 and 7.

For lamps, the reported value shall be the average measured values of the tested units rounded to be the nearest tenth.

For all other sources, the reported value shall be the minimum power factor of the tested units rounded to the nearest tenth.

### JA8.3.3 Start Time Test

Start time shall be measured in accordance with the ENERGY STAR Program Requirements Product Specifications for Lamps 1.1: Start Time Test Method, notwithstanding the scope of the test.

For lamps the reported value shall be the average start time of the tested units rounded to the nearest millisecond.

For all other sources the reported value shall be the maximum start time of the tested units rounded to the nearest millisecond.

### JA8.3.4 Color Characteristics Tests

Correlated Color Temperature (CCT), Duv, and Color Rendering Index shall be determined by the following test procedures, as applicable to the type of light source:

a) Incandescent and halogen reflector lamps: IES LM-20.

b) Incandescent non-reflector lamps: IES LM-45.

c) General service fluorescent lamps: 10CFR 430.23(r).

d) Single ended compact fluorescent lamps: IES LM-66.

e) Fluorescent lamps that are not single ended compact fluorescent lamps or general service fluorescent lamps: IES LM-9.

f) Induction lamps: IES LM-66.

g) LED light sources: IES LM 79.

h) High intensity discharge lamps: IES LM-51.

i) Other applicable test procedure approved by the Executive Director

Correlated Color Temperature (CCT) and Duv shall be calculated in accordance with CIE 15 (reference document ANSI C78.377). Color Rendering Index (CRI) shall be calculated in accordance with CIE 13.3.

The reported value shall be the average measured values of units tested rounded to be the nearest whole number for CCT and CRI and to 4 decimal places (closest ten thousandth) for Duv.

### JA8.3.5 Ambient Temperature Life Test

The following light sources shall be tested in accordance with the ENERGY STAR Product Specification for Lamps Version 1.1: Ambient Temperature Life Testing, in an ambient temperature condition between 20°C and 35°C and satisfy the lumen maintenance and 6,000 hour survival rate criteria:

a) Omnidirectional lamps < 10 watts, and decorative lamps for which the manufacturer has not performed an elevated temperature life test to show compliance with lumen maintenance requirements in this specification;

b) Omnidirectional lamps labeled “not for use in enclosed fixtures” on the lamp ;

c) LED light engines and lamps labeled “not for use in recessed fixtures” on the product ; and

d) Inseparable SSL luminaire: Alternatively inseparable SSL luminaires may reference the in-situ measurement temperature of the LED, IES LM80 test results and TM21 projections for the light source used in the luminaire.

(j)

For lamps the reported value shall be the 9th highest measured lumen maintenance value measured (9 out of 10 units must pass life testing).

For all other sources (except those using the IES-LM80 test method and the IES-TM21 calculation method for projecting lumen maintenance) the reported value shall be the minimum measured lumen maintenance value of the 3 samples.

(k)

Inseparable SSL luminaires designed to be recessed, shall be ICAT (insulation contact air tight) rated in accordance with Section 150.0(k)1C and tested with sides and top of luminaire in direct contact of least 12" of R-38 fiberglass insulation.

For inseparable SSL luminaires referencing the in-situ measurement temperature of the LED, IES -LM80 test results and projecting lumen maintenance using the IES-TM21 calculation method for the light source used in the luminaire, ten samples for each TS and drive current combination (refer to IES TM-21, section 4.2) must be tested. Each sample set may be composed entirely of one nominal CCT, or may be split between no more than two adjacent nominal CCT values as outlined in ANSI C78.377 (e.g. 2700 and 3000K). Passing Test: all of the conditions below shall be met.

1. In the sample luminaire, the in situ TMPLED temperature is less than or equal to the temperature specified in the LM-80 test report for the corresponding or higher drive current, within the manufacturer’s specified operating current range.

2. The drive current measured in the luminaire is less than or equal to the drive current specified in the LM-80 test report at the corresponding temperature or higher.

3. The TM-21 lumen maintenance life projection report projects an L70 meeting or exceeding requirements.

### JA8.3.6 Elevated Temperature Life Test

The following light sources shall be tested in accordance with the ENERGY STAR Product Specification for Lamps Version 1.1: Elevated Temperature Life Testing.

a) Omnidirectional lamps ≥ 10 Watts that are not labeled "not for use in enclosed fixtures" or "not for use in recessed fixtures"; and

b) All other light sources that are not inseparable SSL luminaires, and that are not labeled "not for use in enclosed fixtures" or "not for use in recessed fixtures."

(l)

The Option A test method ENERGY STAR Elevated Temperature Life Test shall be modified as follows: Light source shall be tested in an ICAT (insulation contact, air-tight) recessed luminaire of the appropriate size for the source under test. The ICAT luminaire shall be listed for zero clearance insulation contact (IC) by Underwriters Laboratories or other nationally recognized testing/rating laboratory and have a label that certifies that the luminaire is airtight with air leakage less than 2.0 CFM at 75 Pascals when tested in accordance with ASTM E283. The sides and top of ICAT recessed luminaire shall be in direct contact of least 12" of R-38 fiberglass insulation.

Light sources tested in accordance with the ENERGY STAR Elevated Temperature Life Test, notwithstanding scope, shall use the modified Option A test method as described above or Option B or C with an operating temperature of:

45degC +/-5degC for omnidirectional sources between 10 and 20 Watts;

45degC +/-5degC for all sources other than omnidirectional not greater than 20 Watts;

55degC +/-5degC for all sources greater than 20 Watts.

(m)

If units are tested both base-up and base-down, the average of surviving unit measured values shall be calculated for each orientation and the reported lumen maintenance shall be the lesser of the two averages rounded to the nearest tenth of a percent if the difference between the averages is greater than 3%; if less than 3% difference, then the reported lumen maintenance shall be the average of all surviving units rounded to the nearest tenth percent. If units are tested in one orientation, the reported lumen maintenance value shall be the average of surviving unit measured values rounded to the nearest tenth percent.

(n)

(o) For all other sources the reported value shall be the minimum measured lumen maintenance value of the three samples.

JA8.3.7 Tests for Minimum Dimming Level, Flicker, and Audible Noise

The flicker test is performed for light sources as specified in Joint Appendix JA10 and the audible noise test as specified in the ENERGY STAR Program Requirements Product Specification for Lamps Version 1.1: Noise Recommended Practices, notwithstanding scope.

Minimum dimming level is measured by comparing the stabilized light output of the light source with the dimming control set to full light output with the dimming control being set to the manufacturer’s minimum rated output. Full light output and minimum light output is measured after the light output has stabilized according to the test procedures specific to light source type in Section JA 8.3.1.

In addition to the reporting of flicker results as described in Section JA8.6, flicker test data for each combination of light source, ballast or driver (if applicable), transformer type and dimmer type claiming compliance with JA8 shall be submitted to the California Energy Commission in the format as defined in Joint Appendix JA10.

Testing for minimum dimming level, flicker, and audible noise is required for each combination of light source, ballast or driver (if applicable), transformer type and dimmer type as follows:

1. Low voltage light sources shall be tested with a representative transformer for each transformer type that the light source is claiming compatibility.

2. Light sources claimed as compatible with forward phase-cut dimmers shall be tested in combination with a NEMA SSL 7A compliant dimmer.

3. Light sources claimed as compatible with dimmers other than forward phase-cut dimmers, dimmability, low noise and low flicker operation shall be tested for each ballast or driver combination (if applicable) with at least one representative dimmer for each dimmer type for which compatibility is claimed.