# Appendix B: Excerpts from the Appliance Efficiency Regulations

#### Table T-1
Normal Impedance Ranges for Liquid-Immersed Transformers

Single‐phase | Three‐phase
kVA | Impedance (%) | kVA | Impedance (%)
10 | 1.0–4.5 | 15 | 1.0–4.5
15 | 1.0–4.5 | 30 | 1.0–4.5
25 | 1.0–4.5 | 45 | 1.0–4.5
37.5 | 1.0–4.5 | 75 | 1.0–5.0
50 | 1.5–4.5 | 112.5 | 1.2–6.0
75 | 1.5–4.5 | 150 | 1.2–6.0
100 | 1.5–4.5 | 225 | 1.2–6.0
167 | 1.5–4.5 | 300 | 1.2–6.0
250 | 1.5–6.0 | 500 | 1.5–7.0
333 | 1.5–6.0 | 750 | 5.0–7.5
500 | 1.5–7.0 | 1000 | 5.0–7.5
667 | 5.0–7.5 | 1500 | 5.0–7.5
833 | 5.0–7.5 | 2000 | 5.0–7.5
|  | 2500 | 5.0–7.5

#### Table T-2
Normal Impedance Ranges for Dry-Type Transformers

Single‐phase | Three‐phase
kVA | Impedance (%) | kVA | Impedance (%)
15 | 1.5–6.0 | 15 | 1.5–6.0
25 | 1.5–6.0 | 30 | 1.5–6.0
37.5 | 1.5–6.0 | 45 | 1.5–6.0
50 | 1.5–6.0 | 75 | 1.5–6.0
75 | 2.0–7.0 | 112.5 | 1.5–6.0
100 | 2.0–7.0 | 150 | 1.5–6.0
167 | 2.5–8.0 | 225 | 3.0–7.0
250 | 3.5–8.0 | 300 | 3.0–7.0
333 | 3.5–8.0 | 500 | 4.5–8.0
500 | 3.5–8.0 | 750 | 5.0–8.0
667 | 5.0–8.0 | 1000 | 5.0–8.0
833 | 5.0–8.0 | 1500 | 5.0–8.0
|  | 2000 | 5.0–8.0
|  | 2500 | 5.0–8.0

#### Table A-1
Non-Commercial Refrigerator, Refrigerator-Freezer, and Freezer Test Methods

Appliance | Test Method
Non‐commercial refrigerators, designed for the refrigerated storage of food at temperatures above 32°F and below 39°F, refrigerated food storage; refrigerator‐freezers; and freezers. | 10 C.F.R. sections 430.23(a) (Appendix A to Subpart B of part 430) and 430.23(b) (Appendix B to Subpart B of part 430)
Wine chillers that are consumer products | 10 C.F.R. section 430.23(a) (Appendix A1 to Subpart B of part 430), with the following modifications: Standardized temperature as referred to in Section 3.2 of Appendix A1 shall be 55°F (12.8°C). The calculation of test ’cycle energy expended (ET) in section 5.2.1.1 of Appendix A1 shall be made using the modified formula: ET=(EP x 1440 x k)/T Where k = 0.85

#### Table A-2
Commercial Refrigerator, Refrigerator-Freezer, and Freezer Test Methods

Appliance | Test Method
Automatic commercial ice makers | 10 C.F.R. sections 431.133 and 431.134
Refrigerated bottled or canned beverage vending machines | 10 C.F.R. sections 431.293 and 431.294
Refrigerated buffet and preparation tables | ANSI/ASTM F2143‐01
Other commercial refrigerators, ‘refrigerator‐freezers, and ‘freezers, with doors | 10 C.F.R. sections 431.63 and 431.64
Other commercial refrigerators, refrigerator‐freezers, and freezers, without doors | 10 C.F.R. sections 431.63 and 431.64
Walk‐in coolers and walk‐in freezers | 10 C.F.R. sections 431.303 and 431.304

#### Table B-1
Room Air Conditioner, Room Air-Conditioning Heat Pump,
Packaged Terminal Air Conditioner, and Packaged Terminal Heat Pump Test Methods

Appliance | Test Method
Room air conditioners and room air‐conditioning heat pumps | 10 C.F.R. section 430.23(f) (Appendix F to Subpart B of part 430)
Packaged terminal air conditioners and packaged terminal heat pumps | 10 C.F.R. sections 431.95 and 431.96

#### Table C-1
Central Air Conditioner Test Methods

Appliance | Test Method
Computer Room Air Conditioners
evaporatively‐cooled | ANSI/ASHRAE 127‐2001 10 C.F.R. sections 431.95 and 431.96
air‐cooled, glycol‐cooled, water‐cooled
Other electric‐powered unitary air‐conditioners and electric powered heat pumps
Air‐cooled air conditioners and air‐source heat pumps
< 65,000 Btu/hr, single‐phase | 10 C.F.R. section 430.23(m) (Appendix M to Subpart B of part 430)
< 65,000 Btu/hr, three‐phase | 10 C.F.R. sections 431.95 and 431.96
≥ 65,000 and < 760,000 Btu/hr | 10 C.F.R. sections 431.95 and 431.96
evaporatively‐cooled air conditioners < 240,000 Btu/h | 10 C.F.R. sections 431.95 and 431.96
water‐cooled air conditioners and water‐source heat pumps<240,000 Btu/hr | 10 C.F.R. sections 431.95 and 431.96
ground ’water‐source heat pumps | ARI/ISO‐13256‐1:1998
ground‐source closed‐loop heat pumps | ARI/ISO‐13256‐1:1998
Variable Refrigerant Flow Multi‐split Systems | 10 C.F.R. sections 431.95 and 431.96
Single Package Vertical Air Conditioners and Single Package Vertical Heat Pumps | 10 C.F.R. sections 431.95 and 431.96
’Gas‐fired ‘air conditioners and gas‐fired heat pumps | ANSI Z21.40.4‐1996 as modified by CEC, Efficiency Calculation Method for Gas‐Fired Heat Pumps as a New Compliance Option (1996)

#### Table D-1
Spot Air Conditioner, Ceiling Fan, Ceiling Fan Light Kit, Evaporative Cooler,
Whole House Fan, Residential Exhaust Fan, and Dehumidifier Test Methods

Appliance | Test Method
Spot ’Air Conditioners | ANSI/ASHRAE 128‐2001
Ceiling Fans, Except Low‐Profile Ceiling Fans | 10 C.F.R. section 430.23(w) (Appendix U to Subpart B of part 430)
Ceiling Fan Light Kits | 10 C.F.R. section 430.23(x) (Appendix V to Subpart B of part 430)
Evaporative Coolers | ANSI/ASHRAE 133‐2008 for packaged direct evaporative coolers and packaged indirect/direct evaporative coolers; ANSI/ASHRAE 143‐2007 for packaged indirect evaporative coolers
Whole House Fans | HVI‐Publication 916, 29 September 2015 HVI Airflow Test Procedure, as specified in section 5.2 Use setups for whole house comfort ventilatiors.
Dehumidifiers | 10 C.F.R. section 430.23(z) (Appendix X to Subpart B of part 430, active mode portion only)
Residential Exhaust Fans | HVI‐Publication 916, 29 September 2015 HVI Airflow Test Procedure, as specified in section 5.2
Residential Furnace Fans | 10 C.F.R. section 430.23(cc) (Appendix AA to Subpart B of part 430)

#### Table E-1
Vented gas space heaters and vented oil space heaters, vented and unvented infrared gas heaters,
electric residential boilers, and gas‐fired combination space‐heating and water‐heating appliances Test Methods

Appliance | Test Method
Central furnaces
< 225,000 Btu/hr, single phase | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430)
< 225,000 Btu/hr, three phase | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430) or 10 C.F.R. sections 431.75 and 431.76 (at manufacturer’s option)
≥ 225,000 Btu/hr | 10 C.F.R. sections 431.75 and 431.76
‘Gas infrared heaters
patio heaters | ASTM F2644‐07
gas‐fired high‐intensity infrared heaters | ANSI Z83.19‐2001
gas‐fired low‐intensity infrared heaters | ANSI Z83.20‐2001
Unit heaters
gas‐fired | ANSI Z83.8‐2002*
oil‐fired | UL 731‐1995*
Gas duct furnaces | ANSI Z83.8‐2002
Boilers
< 300,000 Btu/hr | 10 C.F.R. section 430.23(n) (Appendix N to Subpart B of part 430)
≥ 300,000 Btu/hr | 10 C.F.R. sections 431.85 and 431.86
Wall furnaces, floor furnaces, and room heaters | 10 C.F.R. section 430.23(o) (Appendix O to Subpart B of part 430)
*To calculate maximum energy consumption during standby, measure the gas energy used in one hour (in Btus) and the electrical energy used (in watt‐hours) over a one‐hour period, when the main burner is off. Divide Btus and watt‐hours by one hour to obtain Btus per hour and watts. Divide Btus per hour by 3.412 to obtain watts. Add watts of gas energy to watts of electrical energy to obtain standby energy consumption in watts.

#### Table F-1
Small Water Heater Test Methods

Appliance | Test Method
Small water heaters that are federally‐regulated consumer products | 10 C.F.R. part 430, Subpart B, Appendix E, section 5: “Test Procedures” and part 430.23(e)(4): “The alternative uniform test method for measuring the energy consumption of untested water heaters shall be that set forth in section 7.0 of Appendix E of this subpart.”
Small water heaters that are not federally‐regulated consumer products
’Gas and oil storage‐type < 20 gallons rated capacity | ANSI/ASHRAE 118.2‐1993
Booster water heaters | ANSI/ASTM F2022‐00 (for all matters other than volume) ANSI Z21.10.3‐1998 (for volume)
Hot ’water dispensers | Test Method in 1604(f)(4)
Mini‐tank electric water heaters | Test Method in 1604(f)(5)
All others | 10 C.F.R. section 430.23(e) (Appendix E to Subpart B of part 430)

#### Table G-1
Pool Heater Test Methods

Appliance | Test Method
’Gas‐fired and oil‐fired ’pool heaters | 10 C.F.R. section 430.23(p) (Appendix P to Subpart B of part 430)
Electric resistance ‘pool heaters | ANSI/ASHRAE 146‐1998
Heat pump pool heaters | ANSI/ASHRAE 146‐1998, as modified by Addendum Test Procedure published by Pool Heat Pump Manufacturers Association dated April, 1999, Rev 4: Feb. 28, 2000:
Reading | Standard Temperature Rating | Low‐Temperature Rating | Spa Conditions Rating
Air Temperature Dry‐bulb Wet‐bulb | 27.0°C (80.6°F) 21.7°C (71.0°F) | 10.0°C (50.0°F) 6.9°C (44.4°F) | 27.0°C (80.6°F) 21.7°C (71.0°F)
Relative Humidity | 63% | 63% | 63%
Pool Water Temperature | 26.7°C (80.0°F) | 26.7°C (80.0°F) | 40.0°C (104.0°F)

#### Table R-1
Cooking Product and Food Service Equipment Test Methods

Appliance | Test Method
Cooking products that are consumer products | 10 C.F.R. section 430.23(i) (Appendix I to Subpart B of part 430)
Commercial hot food holding cabinets | ANSI/ASTM F2140-01 (Test for idle energy rate-dry test) and US EPA’s Energy Star Guidelines, “Measuring Interior Volume” (Test for interior volume)
Commercial convection ovens | ANSI/ASTM F1496-99 (Test for energy input rate and idle energy consumption only)
Commercial range tops | ANSI/ASTM F1521-96 (Test for cooking energy efficiency only)

#### Table A-3
Standards for Non-Commercial Refrigerators, Refrigerator-Freezers, and Freezers

Appliance | Defrost | Compact, Built‐ in, Neither | Ice | Maximum Energy Consumption (kWh/year)
Equipped with Automatic Ice Maker? | Dispense Ice Through Door? | July 1, 20011 | Sept. 15, 20142
Refrigerators
Not ‘all refrigerator’ | Manual | Neither | ‐‐ | ‐‐ | 8.82AV + 248.4 | 7.99AV + 225.0
Not ‘all refrigerator’ | Manual | Compact | ‐‐ | ‐‐ | 10.70AV + 299.0 | 9.03AV + 252.3
‘All refrigerator’ | Manual | Compact | ‐‐ | ‐‐ | 10.70AV + 299.0 | 7.84AV + 219.1
‘All refrigerator’ | Manual | Neither | ‐‐ | ‐‐ | ‐‐ | 6.79AV + 193.6
‘All refrigerator’ | Automatic | Neither | ‐‐ | ‐‐ | 9.80AV + 276.0 | 7.07AV + 201.6
‘All refrigerator’ | Automatic | Built‐in | ‐‐ | ‐‐ | ‐‐ | 8.02AV + 228.5
‘All refrigerator’ | Automatic | Compact | ‐‐ | ‐‐ | 12.70AV + 355.0 | 9.17AV + 259.3
Refrigerator‐freezers
| Manual | Neither | ‐‐ | ‐‐ | 8.82AV + 248.4 | 7.99AV + 225.0
Partial | Neither | ‐‐ | ‐‐ | 8.82AV + 248.4 | 7.99AV + 225.0
Manual | Compact | ‐‐ | ‐‐ | ‐‐ | 9.03AV + 252.3
Partial | Compact | ‐‐ | ‐‐ | 7.00AV + 398.0 | 5.91AV + 335.8
Refrigerator‐‘freezers Bottom‐‘Freezer
| Automatic | Neither | No | ‐‐ | 4.60AV + 459.0 | 8.85AV + 317.0
Automatic | Neither | Yes | No | ‐‐ | 8.85AV + 401.0
Automatic | Neither | Yes | Yes | ‐‐ | 9.25AV + 475.4
Automatic | Compact | No | ‐‐ | 13.10AV + 367.0 | 11.80AV + 339.2
Automatic | Compact | Yes | ‐‐ | ‐‐ | 11.80AV + 423.2
Automatic | Built‐in | No | ‐‐ | ‐‐ | 9.40AV + 336.9
Automatic | Built‐in | Yes | No | ‐‐ | 9.40AV + 420.9
Automatic | Built‐in | Yes | Yes | ‐‐ | 9.83AV + 499.9
Refrigerator‐freezers Side‐by‐side
| Automatic | Neither | No | ‐‐ | 4.91AV+507.5 | 8.51AV + 297.8
Automatic | Neither | Yes | No | ‐‐ | 8.51AV + 381.8
Automatic | Neither | Yes | Yes | 10.10AV + 406.0 | 8.54AV + 432.8
Automatic | Compact | No | ‐‐ | 7.60AV + 501.0 | 6.82AV + 456.9
Automatic | Compact | Yes | ‐‐ | ‐‐ | 6.82AV + 540.9
Automatic | Built‐in | No | ‐‐ | ‐‐ | 10.22AV + 357.4
Automatic | Built‐in | Yes | No | ‐‐ | 10.22AV + 441.4
Automatic | Built‐in | Yes | Yes | ‐‐ | 10.25AV + 502.6
Refrigerator‐freezers Top‐Freezer
| Automatic | Neither | No | ‐‐ | 9.80AV + 276.0 | 8.07AV + 233.7
| Automatic | Neither | Yes | No | ‐‐ | 8.07AV + 317.7
| Automatic | Neither | Yes | Yes | 10.20AV + 356.0 | 8.40AV + 385.4
| Automatic | Compact | No | ‐‐ | 12.70AV + 355.0 | 11.80AV + 339.2
¹AV = adjusted total volume, expressed in ft3, as determined in 10 C.F.R., part 430, Appendices A1 and B1 of Subpart B, which is: [1.44 x freezer volume (ft3)] + refrigerator volume (ft3) for refrigerators; [1.63 x freezer volume (ft3)] + refrigerator volume (ft3) for refrigerator‐freezers; [1.73 x freezer volume (ft3)] for freezers. ²AV = adjusted total volume, expressed in ft3, as determined in 10 C.F.R., part 430, Appendices A and B of Subpart B.
|  |  |  |  |  |  |  |

#### Table A-4
Standards for Commercial Refrigerators, Refrigerator-Freezers
with a Self-Contained Condensing Unit That are Not Commercial Hybrid Units

Equipment Category and Effective Date | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers Effective January 1, 2010 Effective January 1, 2012 | Self Contained (SC) | Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, SC, M VCT, SC, L | 0.12 × V + 3.34 0.75 × V + 4.10
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, SC, M HCT, SC, L | 0.12 × V + 3.34 0.75 × V + 4.10
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, SC, M VCS, SC, L | 0.10 × V + 2.04 0.40 × V + 1.38
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, SC, M HCS, SC, L | 0.10 × V + 2.04 0.40 × V + 1.38
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, SC, M SOC, SC, L | 0.12 × V + 3.34 0.6 TDA + 1.0 0.75 × V + 4.10
Refrigerators with transparent doors designed for pull-down temperature applications. Effective January 1, 2010 | Self Contained (SC) | Vertical Closed Transparent (VCT) | 38 (P) | ≥ 32 | VCT, SC, P | 0.126 × V + 3.51
Horizontal Closed Transparent (HCT) | 38 (P) | ≥ 32 | HCT, SC, P | 0.126 × V + 3.51
Refrigerators and Freezers without Doors Effective January 1, 2012 | Self Contained (SC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, SC, M VOP, SC, L | 1.74 × TDA + 4.71 4.37 × TDA +11.82
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, SC, M SVO, SC, L | 1.73 × TDA + 4.59 4.34 × TDA +11.51
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, SC, M HZO, SC, L | 0.77 × TDA + 5.55 1.92 × TDA + 7.08
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.
|  |  |  |  |  |  |  |

#### Table A-5
Standards for Commercial Refrigerators and Freezers
with a Remote Condensing Unit That are Not Commercial Hybrid Units

Equipment Category | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers Effective January 1, 2012 | ‘Remote (RC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, RC, M VOP, RC, L | 0.82 × TDA + 4.07 2.27 × TDA + 6.85
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, RC, M SVO, RC, L | 0.83 × TDA + 3.18 2.27 × TDA + 6.85
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, RC, M HZO, RC, L | 0.35 × TDA + 2.88 0.57 × TDA + 6.88
Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, RC, M VCT, RC, L | 0.22 × TDA + 1.95 0.56 × TDA + 2.61
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, RC, M HCT, RC, L | 0.16 × TDA + 0.13 0.34 × TDA + 0.26
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, RC, M VCS, RC, L | 0.11 × V + 0.26 0.23 × V + 0.54
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, RC, M HCS, RC, L | 0.11 × V + 0.26 0.23 × V + 0.54
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, RC, M SOC, RC, L | 0.51 × TDA + 0.11 1.08 × TDA + 0.22
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.

#### Table A-7
Standards for Automatic Commercial Ice Makers Manufactured on or After January 1, 2010

Equipment type | Type of cooling | Harvest rate (lbs ice/24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (gal/100 lbs ice)
Ice Making Head | Water | < 500 | 7.80–0.0055H | 200–0.022H.
Ice Making Head | Water | ≥ 500 and < 1436 | 5.58–0.0011H | 200–0.022H.
Ice Making Head | Water | ≥ 1436 | 4.0 | 200–0.022H.
Ice Making Head | Air | < 450 | 10.26–0.0086H | Not applicable.
Ice Making Head | Air | ≥ 450 | 6.89–0.0011H | Not applicable.
Remote Condensing (but not remote compressor) | Air | < 1000 | 8.85–0.0038H | Not applicable.
Remote Condensing (but not remote compressor) | Air | ≥ 1000 | 5.1 | Not applicable.
Remote Condensing and Remote Compressor | Air | < 934 | 8.85–0.0038H | Not applicable.
Remote Condensing and Remote Compressor | Air | ≥ 934 | 5.3 | Not applicable.
Self Contained | Water | < 200 | 11. 40–0.019H | 191–0.0315H.
Self Contained | Water | ≥ 200 | 7.6 | 191–0.0315H.
Self Contained | Air | < 175 | 18.0–0.0469H | Not applicable.
Self Contained | Air | ≥ 175 | 9.8 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

#### Table B-2
Standards for Room Air Conditioners and Room Air-Conditioning
Heat Pumps Manufactured on or After October 1, 2000 and Before June 1, 2014

Appliance | Louvered Sides | Cooling Capacity (Btu/hr) | Minimum EER
Room ‘Air Conditioner | Yes | < 6,000 | 9.7
Room Air Conditioner | Yes | > 6,000 – 7,999 | 9.7
Room Air Conditioner | Yes | > 8,000 – 13,999 | 9.8
Room Air Conditioner | Yes | > 14,000 – 19,999 | 9.7
Room Air Conditioner | Yes | > 20,000 | 8.5
Room Air Conditioner | No | < 6,000 | 9.0
Room Air Conditioner | No | > 6,000 – 7,999 | 9.0
Room Air Conditioner | No | > 8,000 – 19,999 | 8.5
Room Air Conditioner | No | > 20,000 | 8.5
Room Air Conditioning Heat Pump | Yes | < 20,000 | 9.0
Room Air Conditioning Heat Pump | Yes | > 20,000 | 8.5
Room Air Conditioning Heat Pump | No | < 14,000 | 8.5
Room Air Conditioning Heat Pump | No | > 14,000 | 8.0
Casement‐Only Room Air Conditioner | Either | Any | 8.7
Casement‐Slider Room Air Conditioner | Either | Any | 9.5

#### Table B-3
Standards for Room Air Conditioners and Room Air-Conditioning
Heat Pumps Manufactured On or After June 1, 2014

Appliance | Louvered Sides | Cooling Capacity (Btu/hr) | Minimum Combined EER
Room ‘Air Conditioner | Yes | < 6,000 | 11.0
Room Air Conditioner | Yes | > 6,000 – 7,999 | 11.0
Room Air Conditioner | Yes | > 8,000 – 13,999 | 10.9
Room Air Conditioner | Yes | > 14,000 – 19,999 | 10.7
Room Air Conditioner | Yes | > 20,000 – 27,999 | 9.4
Room Air Conditioner | Yes | > 28,000 | 9.0
Room Air Conditioner | No | < 6,000 | 10.0
Room Air Conditioner | No | > 6,000 – 7,999 | 10.0
Room Air Conditioner | No | > 8,000 – 10,999 | 9.6
Room Air Conditioner | No | > 11,000 – 13,999 | 9.5
Room Air Conditioner | No | > 14,000 – 19,999 | 9.3
Room Air Conditioner | No | > 20,000 | 9.4
Room Air Conditioning Heat Pump | Yes | < 20,000 | 9.8
Room Air Conditioning Heat Pump | Yes | > 20,000 | 9.3
Room Air Conditioning Heat Pump | No | < 14,000 | 9.3
Room Air Conditioning Heat Pump | No | > 14,000 | 8.7
Casement‐Only Room Air Conditioner | Either | Any | 9.5
Casement‐Slider Room Air Conditioner | Either | Any | 10.4

#### Table C-3
Standards for Single Phase Air-Cooled Air Conditioners with Cooling Capacity
Less than 65,000 Btu per Hour and Single Phase Air-Source Heat Pumps
with Cooling Capacity Less than 65,000 Btu per Hour, Not Subject to EPAct

Appliance | Minimum ‘Efficiency
Effective January 23, 2006 | Effective January 1, 2015
Minimum SEER | Minimum HSPF | Minimum SEER | Minimum HSPF | Minimum EER | Average Off‐ Mode Power Consumption Pw. pff (watts)
Split system ‘air conditioners with rated cooling capacity < 45,000 Btu/hour¹ | 13.0 | — | 14.0 | — | 12.2 | 30
Split system air conditioners with rated cooling capacity ≥ 45,000 Btu/hour¹ | 14.0 | — | 11.7 | 30
Split system ‘heat pumps | 13.0 | 7.7 | 14.0 | 8.2 | — | 33
Single package air conditioners¹ | 13.0 | — | 14.0 | — | 11.0 | 30
Single package heat pumps | 13.0 | 7.7 | 14.0 | 8.0 | — | 33
Space constrained air conditioners – split system | 12.0 |  | 12.0 | — | — | 30
Space constrained heat pumps – split system | 12.0 | 7.4 | 12.0 | 7.4 | — | 33
Space constrained air conditioners – single package | 12.0 |  | 12.0 | — | — | 30
Space constrained heat pumps – single package | 12.0 | 7.4 | 12.0 | 7.4 | — | 33
Small duct, high velocity ‘air conditioner systems | 13.0 |  | 13.0 | — | — | 30
Small duct, high velocity ‘heat pump systems | 13.0 | 7.7 | 13.0 | 7.7 | — | 30
¹ See 10 C.F.R. section 430.32(c) for less stringent federal standards applicable to these units that are manufactured on or after January 1, 2015 and installed in states other than Arizona, California, Nevada, or New Mexico

#### Table C-4
Standards for Air-Cooled Air Conditioners and Air-Source Heat Pumps Subject to EPAct
(Standards Effective January 1, 2010 Do Not Apply To Single Package Vertical Air Conditioners)

Appliance | Cooling Capacity (Btu/hr) | System Type | Minimum ‘Efficiency
Effective June 15, 2008 | Effective January 1, 2010
Air Conditioners | Heat Pumps
Air‐cooled unitary air conditioners and heat pumps (cooling mode) | < 65,000 * | Split system | 13.0 SEER |  |
< 65,000 * | Single package | 13.0 SEER |  |
≥ 65,000 and< 135,000 | All | 11.0 EER4 | 11.2 EER³ 10.8 EER4 | 11.0 EER³
≥ 135,000 and< 240,000 | All |  | 11.0 EER³ 10.8 EER4 | 10.6 EER³ 10.4 EER4
≥ 240,000 and< 760,000 | All |  | 10.0 EER³ 9.8 EER4 | 9.5 EER³ 9.3 EER4
Air‐cooled unitary air conditioning heat pumps (heating mode) | < 65,000 * | Split system | 7.7 HSPF |
< 65,000 * | Single package | 7.7 HSPF |
≥ 65,000 and< 135,000 | All |  | 3.3 COP
≥ 135,000 and< 240,000 | All |  | 3.2 COP
≥ 240,000 and< 760,000 | All |  | 3.2 COP
* Three phase models only. ³ Applies to equipment that has electric resistance heat or no heating. 4 Applies to equipment with all other heating‐system types that are integrated into the unitary equipment.

#### Table C-5
Standards for Water-Cooled Air Conditioners, Evaporatively Cooled
Air Conditioners, and Water-Source Heat Pumps

Appliance | Cooling Capacity (Btu per hour) | Minimum ‘Efficiency
Effective Prior to October 29, 2012 | Effective January 10, 2011 | Effective †October 29, 2012 or ††October 29, 2013 | Effective *June 1, 2013 or**June 1, 2014
Minimum EER COP | Minimum EER COP | Minimum EER …COP | Minimum EER COP
Water-cooled ‘air conditioners and evaporatively cooled air conditioners | < 17,000 | 12.1 |  |  |
Water-source ‘heat pumps | < 17,000 | 11.2 | 11.2 4.2 |  |  |
Water-source VRF multi-split heat pumps | < 17,000 | — | 4.2 |  | 12.0¹† | 4.2 |
Water-cooled air conditioners and evaporatively cooled air conditioners | > 17,000 and < 65,000 | 12.1 | 12.1 |  |  |
Water-source heat pumps, including VRF | > 17,000 and < 65,000 | 12.0 | 12.0 4.2 |  |  |
Water-cooled air conditioners and evaporatively cooled air conditioners | > 65,000 and < 135,000 | 11.5¹ | 11.51 |  |  | 12.1¹* —
Water-source heat pumps, including VRF | > 65,000 and < 135,000 | 12.0 | 12.0 4.2 |  |  | 11.9* 4.2
Water-cooled air conditioners | > 135,000 and < 240,000 | 11.0 | 11.0 |  |  | 12.5¹** —
Evaporatively cooled air conditioners | > 135,000 and < 240,000 | 11.0 | 11.0 |  |  | 12.0¹** —
Water-source heat pumps | > 135,000 and < 240,000 | 11.0 | 11.0 2.9 |  |  | 12.3** 2.9
Water-source VRF multi-split heat pumps | > 135,000 and < 760,000 |  |  | 10.0¹†† 3.9†† |
Water-cooled air conditioners | > 240,000 and < 760,000 | 11.0¹ | 11.0¹ |  | 12.4*** —
Evaporatively cooled air conditioners | > 240,000 and < 760,000 | 11.0¹ | 11.0¹ |  | 11.9*** —
Water-source heat pumps | > 240,000 and < 760,000 | 11.0¹ | 11.0¹ |  | 12.2** —
¹ Deduct 0.2 from the required EER for units with heating sections other than electric resistance heat. For VRF multi-split heat pumps this applies to units with heat recovery.
|  |  |  |  |  |  |  |

#### Table C-6
Standards for Single Package Vertical Air Conditioners and Single Package Vertical Heat Pumps Manufactured on or After January 1, 2010

Appliance | Cooling Capacity (BTU/hr) | System Type | Minimum ‘Efficiency
Cooling Mode | Heating Mode
Single package vertical ‘air conditioners | < 65,000 | Single‐phase | 9.0 EER | N/A
< 65,000 | 3‐phase | 9.0 EER | N/A
≥ 65,000 and < 135,000 | All | 8.9 EER | N/A
≥ 135,000 and < 240,000 | All | 8.6 EER | N/A
Single package vertical ‘heat pumps | < 65,000 | Single‐phase | 9.0 EER | 3.0 COP
< 65,000 | 3‐phase | 9.0 EER | 3.0 COP
≥ 65,000 and < 135,000 | All | 8.9 EER | 3.0 COP
≥ 135,000 and < 240,000 | All | 8.6 EER | 2.9 COP

#### Table D-2
Standards for Dehumidifiers

Product capacity (pint/day) | Minimum energy factor (liters/kWh)
Effective October 1, 2007 | Effective October 1, 2012
25.00 or less | 1.00 | 1.35
25.01 – 35.00 | 1.20 | 1.35
35.01 – 45.00 | 1.30 | 1.50
45.01 – 54.00 | 1.30 | 1.60
54.01 – 74.99 | 1.50 | 1.70
75.00 or more | 2.25 | 2.50

#### Table E-2
Standards for Gas Wall Furnaces, Floor Furnaces, and Room Heaters

Appliance | Design Type | Capacity (Btu per hour) | Minimum AFUE (%)
Effective Before April 16, 2013 | Effective On or After April 16, 2013
Wall furnace | Fan | < 42,000 | 73 | 75
Wall furnace | Fan | > 42,000 | 74 | 76
Wall furnace | Gravity | < 10,000 | 59 | 65
Wall furnace | Gravity | > 10,000 and < 12,000 | 60
Wall furnace | Gravity | > 12,000 and < 15,000 | 61
Wall furnace | Gravity | > 15,000 and < 19,000 | 62
Wall furnace | Gravity | > 19,000 and < 27,000 | 63
Wall furnace | Gravity | > 27,000 and < 46,000 | 64 | 66
Wall furnace | Gravity | > 46,000 | 65 | 67
Floor furnace | All | < 37,000 | 56 | 57
Floor furnace | All | > 37,000 | 57 | 58
Room heater | All | < 18,000 | 57 | 61
Room heater | All | > 18,000 and < 20,000 | 58
Room heater | All | > 20,000 and < 27,000 | 63 | 66
Room heater | All | > 27,000 and < 46,000 | 64 | 67
Room heater | All | > 46,000 | 65 | 68

#### Table E-3
Standards for Gas- and Oil-Fired Central Boilers
< 300,000 Btu/hour Input and Electric Residential Boilers

Appliance | Minimum AFUE (%)
Effective January 1, 1992 | Effective September 1, 2012
Gas steam boilers with single phase electrical supply | 75 | 80 ¹
Gas hot ‘water boilers with single phase electrical supply | 80 | 82 ¹,²
Oil steam ‘boilers with single phase electrical supply | — | 82
Oil hot water boilers with single phase electrical supply | — | 84 ²
Electric steam residential boilers | — | NONE
Electric hot water residential boilers |  | NONE ²
All other boilers with single phase electrical supply | 80 | —
Gas ‘packaged boilers | --- | ---
Oil packaged boilers | --- | ---
¹ No constant burning pilot light design standard effective September 1, 2012. ² Automatic means for adjusting temperature design standard effective September 1, 2012. (Boilers equipped with tankless domestic water heating coils do not need to comply with this requirement.)

#### Table E-5
Standards for Commercial Gas- and Oil-Fired Central Furnaces

Appliance | Rated Input (Btu/hr) | Minimum Thermal ‘Efficiency
Gas central furnaces | > 225,000 | 80
Oil central furnaces | > 225,000 | 81

#### Table F-2
Standards for Large Water Heaters Effective October 29, 2003

Appliance | Input to Volume Ratio | Size (Volume) | Minimum Thermal ‘Efficiency (%) | Maximum Standby Loss¹,²
Gas storage water heaters | < 4,000 Btu/hr/gal | Any | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Gas instantaneous water heaters | < 4,000 Btu/hr/gal | < 10 gal | 80 | –
> 10 gal | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Gas hot water supply boilers | < 4,000 Btu/hr/gal | < 10 gal | 80 | –
> 10 gal | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Oil storage water heaters | < 4,000 Btu/hr/gal | any | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Oil instantaneous water heaters | < 4,000 Btu/hr/gal | < 10 gal | 80 | –
> 10 gal | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Oil hot water supply boilers | < 4,000 Btu/hr/gal | < 10 gal | 80 | –
> 10 gal | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Electric storage water heaters | < 4,000 Btu/hr/gal | Any | – | 0.3 + 27/Vm %/hr
¹ Standby loss is based on a 70°F temperature difference between stored water and ambient requirements. In the standby loss equations, Vr is the rated volume in gallons, Vm is the measured volume in gallons, and Q is the nameplate input rate in Btu/hr. ² Water heaters and hot water supply boilers having more than 140 gallons of storage capacity are not required to meet the standby loss requirement if the tank surface is thermally insulated to R‐ 12.5, if a standing pilot light is not installed, and for gas‐ or oil‐fired storage water heaters, there is a flue damper or fan‐assisted combustion.

#### Table F-3
Standards for Small Federally-Regulated Water Heaters

Appliance | Rated Storage Volume (gallons) | Minimum Energy Factor
Effective April 16, 2015
‘Gas-fired storage-type water heaters | ≤ 55 | 0.675−(0.0015 × V)
> 55 | 0.8012−(0.00078 × V)
Oil‐fired water heaters (storage and instantaneous) | Any | 0.68 – (.0019 x V)
Electric ‘storage water heaters (excluding tabletop water heaters) | ≤ 55 | 0.960−(0.0003 × V)
> 55 | 2.057−(0.00113 × V)
Electric tabletop water heaters | Any | 0.93 – (0.00132 x V)
Gas‐fired instantaneous water heaters | Any | 0.82 – (0.0019 x V)
Electric instantaneous water heaters (excluding tabletop water heaters) | Any | 0.93 – (0.00132 x V)
Heat pump water heaters | Any | 0.97 – (.00132 x V)
V = Rated storage volume in gallons.

#### Table H-1
Standards for Plumbing Fittings

Appliance | Maximum Flow Rate
Wash fountains | 2.2xrim space (inches)/20 gpm at 60psi
Metering ‘faucets | 0.25 gallons/cycle 1, 2
Metering faucets for wash fountains | 0.25xrim space (inches)/20 gpm at 60 psi 1, 2
1Sprayheads with independently‐controlled orifices and metered controls. The maximum flow rate of each orifice that delivers a pre‐set volume of water before gradually shutting itself off shall not exceed the maximum flow rate for a metering faucet. 2Sprayheads with collectively‐controlled orifices and metered controls. The maximum flow rate of a sprayhead that delivers a pre‐set volume of water before gradually shutting itself off shall be the product of (a) the maximum flow rate for a metering ‘faucet and (b) the number of component lavatories (rim space of the lavatory in inches (millimeters) divided by 20 inches (508 millimeters)).

#### Table J-1
Standards for Fluorescent Lamp Ballasts and Replacement Fluorescent Lamp Ballasts

Application for Operation of | Ballast Input Voltage | Total Nominal Lamp Watts | Minimum Ballast Efficacy Factor
one F40T12 lamp | 120 or 277 | 40 | 2.29¹ | 1.805²
two F40T12 lamps | 120 | 80 | 1.17¹ | 1.060²
277 | 80 | 1.17¹ | 1.050²
two F96T12 lamps | 120 or 277 | 150 | 0.63¹ | 0.570²
two F96T12HO lamps | 120 or 277 | 220 | 0.39¹ | 0.390²
¹ For fluorescent lamp ballasts manufactured on or after April 1, 2005; sold by the manufacturer on or after July 1, 2005; or incorporated into a luminaire by a luminaire manufacturer on or after April 1, 2006. ² For fluorescent lamp ballasts designed, marked, and shipped as replacement ballasts.

#### Table J-2
Standards for Fluorescent Lamp Ballasts1

Application for Operation of | Ballast Input Voltage | Total Nominal Lamp Watts | Minimum Ballast Efficacy Factor
one F34T12 lamp | 120 or 277 | 34 | 2.61
two F34T12 lamps | 120 or 277 | 68 | 1.35
two F96T12/ES lamps | 120 or 277 | 120 | 0.77
two F96T12HO/ES lamps | 120 or 277 | 190 | 0.42
¹ For fluorescent lamp ballasts manufactured on or after July 1, 2009; sold by the manufacturer on or after October 1, 2009; or fluorescent lamp ballasts incorporated into a luminaire by a luminaire manufacturer on or after July 1, 2010.

#### Table K-2
Standards for Federally-Regulated General Service Fluorescent Lamps
Manufactured Before July 15, 2012

Appliance | Nominal ‘Lamp Wattage | Minimum Color Rendering Index (CRI) | Minimum Average Lamp Efficacy (LPW)
4‐foot medium bi‐pin lamps | > 35 | 69 | 75.0
≤ 35 | 45 | 75.0
2‐foot U‐shaped lamps | > 35 | 69 | 68.0
≤ 35 | 45 | 64.0
8-foot slimline lamps | > 65 | 69 | 80.0
≤ 65 | 45 | 80.0
8‐foot high output lamps | > 100 | 69 | 80.0
≤ 100 | 45 | 80.0

#### Table K-3
Standards for Federally-Regulated General Service Fluorescent Lamps
Manufactured On or After July 15, 2012

Appliance | Correlated Color Temperature | Minimum Average Lamp Efficacy (LPW)
4‐foot medium bipin lamps | ≤ 4,500K | 89
> 4,500K and ≤ 7,000K | 88
2‐foot U‐shaped lamps | ≤ 4,500K | 84
> 4,500K and ≤ 7,000K | 81
8-foot slimline lamps | ≤ 4,500K | 97
> 4,500K and ≤ 7,000K | 93
8‐foot high output lamps | ≤ 4,500K | 92
> 4,500K and ≤ 7,000K | 88
4‐foot miniature bipin standard output | ≤ 4,500K | 86
> 4,500K and ≤ 7,000K | 81
4‐foot miniature bipin high output | ≤ 4,500K | 76
> 4,500K and ≤ 7,000K | 72

#### Table K-4
Standards for Federally-Regulated Incandescent Reflector Lamps
Manufactured Before July 15, 2012

Nominal ‘Lamp Wattage | Minimum Average ‘Lamp Efficacy (LPW)
40‐50 | 10.5
51‐66 | 11.0
67‐85 | 12.5
86‐115 | 14.0
116‐155 | 14.5
156‐205 | 15.0

#### Table K-5
Standards for Federally-Regulated Incandescent Reflector Lamps
Manufactured On or After July 15, 2012

‘Lamp Spectrum | Lamp Diameter (inches) | Rated Voltage | Minimum Average ‘Lamp Efficacy (LPW)1
Standard Spectrum | > 2.5 | ≥ 125 | 6.8 x P0.27
< 125 | 5.9 x P0.27
≤ 2.5 | ≥ 125 | 5.7 x P0.27
< 125 | 5.0 x P0.27
Modified Spectrum | > 2.5 | ≥ 125 | 5.8 x P0.27
< 125 | 5.0 x P0.27
≤ 2.5 | ≥ 125 | 4.9 x P0.27
< 125 | 4.2 x P0.27
1P = Rated Lamp Wattage, in Watts

#### Table K-6
Standards for Medium Base Compact Fluorescent Lamps

Factor | Requirements
‘Lamp Power (Watts) and Configuration¹ | Minimum Efficacy: lumens/watt (Based upon initial lumen data)²
Bare Lamp: Lamp Power < 15 Lamp Power ≥ 15 | 45.0 60.0
Covered Lamp (no reflector) Lamp Power < 15 15 ≥ Lamp Power < 19 19 ≥ Lamp Power < 25 Lamp Power ≥ 25 | 40.0 48.0 50.0 55.0
1,000‐hour Lumen Maintenance | The average of at least 5 lamps must be a minimum 90% of initial (100‐ hour) lumen output @ 1,000 hours of rated life.
Lumen Maintenance | 80% of initial (100‐hour) rating at 40 percent of rated life (per ANSI C78.5 Clause 4.10).
Rapid ‘Cycle Stress Test | Per ANSI C78.5 and IESNA LM‐65 (Clauses 2, 3, 5, and 6) Exception: ‘Cycle times must be 5 minutes on, 5 minutes off. Lamp will be cycled once for every two hours of rated life. At least 5 lamps must meet or exceed the minimum number of ‘cycles.
Average Rated Lamp Life | ≥ 6,000 hours as declared by the manufacturer on the packaging. 80% of rated life, statistical methods may be used to confirm lifetime claims based on sampling performance.
¹ Take performance and electrical requirements at the end of the 100‐hour aging period according to ANSI Standard C78.5. The lamp efficacy shall be the average of the lesser of the lumens per watt measured in the base up and/or other specified positions. Use wattages placed on packaging to select proper specification efficacy in this table, not measured wattage. Labeled wattages are for reference only. ² Efficacies are based on measured values for lumens and wattages from pertinent test data. Wattages and lumens placed on packages may not be used in calculation and are not governed by this specification. For multi‐level or dimmable systems, measurements shall be at the highest setting. Acceptable measurement error is ±3%.

#### Table K-7
Standards for Federally-Regulated General Service Incandescent Lamps

Rated Lumen Ranges | Maximum Rate Wattage | Minimum Rate Lifetime | Effective Date
1490‐2600 | 72 | 1,000 hours | January 1, 2012
1050 – 1489 | 53 | 1,000 hours | January 1, 2013
750 – 1049 | 43 | 1,000 hours | January 1, 2014
310 – 749 | 29 | 1,000 hours | January 1, 2014

#### Table K-8
Standards for Federally-Regulated Modified Spectrum General Service Incandescent Lamps

Rated Lumen Ranges | Maximum Rate Wattage | Minimum Rate Lifetime | Effective Date
1118‐1950 | 72 | 1,000 hours | January 1, 2012
788‐1117 | 53 | 1,000 hours | January 1, 2013
563‐787 | 43 | 1,000 hours | January 1, 2014
232‐562 | 29 | 1,000 hours | January 1, 2014

#### Table K-9
Standards for Federally Regulated Candelabra Base
Incandescent Lamps and Intermediate Base Incandescent Lamps

Lamp Base Type | Maximum Rated Wattage
Candelabra | 60
Intermediate | 40

#### Table M-1
Standards for Traffic Signals for Vehicle and Pedestrian Control

Appliance | Maximum Wattage (at 74°C) | Nominal Wattage (at 25°C)
Traffic Signal Module Type: |
12‐inch; Red Ball | 17 | 11
8‐inch; Red Ball | 13 | 8
12‐inch; Red Arrow | 12 | 9
12‐inch; Green Ball | 15 | 15
8‐inch; Green Ball | 12 | 12
12‐inch; Green Arrow | 11 | 11
Pedestrian Module Type: |
Combination Walking Man/Hand | 16 | 13
Walking Man | 12 | 9
Orange Hand | 16 | 13

#### Table O
Standards for Dishwashers

Appliance | Effective January 1, 2010 | Effective May 30, 2013
Maximum ‘Energy Use (kWh/year) | Maximum ‘Water Use (gallons/cycle) | Maximum ‘Energy Use (kWh/year) | Maximum ‘Water Use (gallons/cycle)
Compact ‘dishwashers | 260 | 4.5 | 222 | 3.5
Standard dishwashers | 355 | 6.5 | 307 | 5.0

#### Table P-1
Standards for Residential Clothes Washers Manufactured
On or After January 1, 2007 and Manufactured Before March 7, 2015

Appliance | Minimum Modified ‘Energy Factor Effective January 1, 2007 | Maximum Water Factor Effective January 1, 2011
Top‐loading compact clothes washers | 0.65 | ‐‐
Top‐loading standard clothes washers | 1.26 | 9.5
Top‐loading, semi‐automatic | N/A¹ | ‐‐
Front‐loading ‘clothes washers | 1.26 | 9.5
Suds‐saving | N/A¹ | ‐‐
¹ Must have an unheated rinse water option.

#### Table P-2
Standards for Residential Clothes Washers Manufactured On or After March 7, 2015

Appliance | Minimum Integrated Modified ‘Energy Factor | Maximum Integrated Water Factor
March 7, 2015 | January1, 2018 | March 7, 2015 | January1, 2018
Top‐loading, Compact | 0.86 | 1.15 | 14.4 | 12.0
Top‐loading, Standard | 1.29 | 1.57 | 8.4 | 6.5
Front‐loading, Compact | 1.13 | 1.13 | 8.3 | 8.3
Front‐loading, Standard | 1.84 | 1.84 | 4.7 | 4.7

#### Table P-3
Standards for Commercial Clothes Washers

Appliance | Minimum Modified ‘Energy Factor | Maximum Water Factor
Effective January 8, 2013
Top-loading clothes washer | 1.6 | 8.5
Front-loading clothes washer | 2.00 | 5.5
| Modified Energy Factor (MEF) Cu. ft./kWh/cycle | Integrated Water factor (IWF) gal./cu./cycle
Effective January 8, 2013
Top-loading clothes washer | 1.35 | 8.8
Front-loading clothes washer | 2.00 | 4.1

#### Table Q-1
Standards for Clothes Dryers Manufactured On or After
May 14, 1994 and Manufactured Before January 1, 2015

Appliance | Minimum Energy Factor (lbs/kWh)
Electric, standard clothes dryers | 3.01
Electric, compact, 120 volt clothes dryers | 3.13
Electric, compact, 240 volt clothes dryers | 2.90
Gas clothes dryers | 2.67

#### Table S-1 Standards for Electric Motors

Motor Horsepower/Standard Kilowatt Equivalent | Minimum Nominal Full-Load Efficiency
Open Motors | Enclosed Motors
6 poles | 4 poles | 2 poles | 6 poles | 4 poles | 2 poles
1/0.75 | 80.0 | 82.5 | . . . | 80.0 | 82.5 | 75.5
1.5/1.1 | 84.0 | 84.0 | 82.5 | 85.5 | 84.0 | 82.5
2/1.5 | 85.5 | 84.0 | 84.0 | 86.5 | 84.0 | 84.0
3/2.2 | 86.5 | 86.5 | 84.0 | 87.5 | 87.5 | 85.5
5/3.7 | 87.5 | 87.5 | 85.5 | 87.5 | 87.5 | 87.5
7.5/5.5 | 88.5 | 88.5 | 87.5 | 89.5 | 89.5 | 88.5
10/7.5 | 90.2 | 89.5 | 88.5 | 89.5 | 89.5 | 89.5
15/11 | 90.2 | 91.0 | 89.5 | 90.2 | 91.0 | 90.2
20/15 | 91.0 | 91.0 | 90.2 | 90.2 | 91.0 | 90.2
25/18.5 | 91.7 | 91.7 | 91.0 | 91.7 | 92.4 | 91.0
30/22 | 92.4 | 92.4 | 91.0 | 91.7 | 92.4 | 91.0
40/30 | 93.0 | 93.0 | 91.7 | 93.0 | 93.0 | 91.7
50/37 | 93.0 | 93.0 | 92.4 | 93.0 | 93.0 | 92.4
60/45 | 93.6 | 93.6 | 93.0 | 93.6 | 93.6 | 93.0
75/55 | 93.6 | 94.1 | 93.0 | 93.6 | 94.1 | 93.0
100/75 | 94.1 | 94.1 | 93.0 | 94.1 | 94.5 | 93.6
125/90 | 94.1 | 94.5 | 93.6 | 94.1 | 94.5 | 94.5
150/110 | 94.5 | 95.0 | 93.6 | 95.0 | 95.0 | 94.5
200/150 | 94.5 | 95.0 | 94.5 | 95.0 | 95.0 | 95.0

#### Table T-3 Standards for Low-Voltage Dry-Type Distribution Transformers

Single phase |  |  | Three phase
kVA | Efficiency (%)¹ |  | kVA |  | Efficiency (%)¹
| Effective January 1, 2007 | Effective January 1, 2016 |  | Effective January 1, 2007 | Effective January 1, 2016
15 | 97.7 | 97.70 | 15 | 97.0 | 97.89
25 | 98.0 | 98.00 | 30 | 97.5 | 98.23
37.5 | 98.2 | 98.20 | 45 | 97.7 | 98.40
50 | 98.3 | 98.30 | 75 | 98.0 | 98.60
75 | 98.5 | 98.50 | 112.5 | 98.2 | 98.74
100 | 98.6 | 98.60 | 150 | 98.3 | 98.83
167 | 98.7 | 98.70 | 225 | 98.5 | 98.94
250 | 98.8 | 98.80 | 300 | 98.6 | 99.02
333 | 98.9 | 98.90 | 500 | 98.7 | 99.14
|  |  | 750 | 98.8 | 99.23
|  |  | 1000 | 98.9 | 99.28
¹ Efficiencies are determined at the following reference conditions: (1) for no-load losses, at the temperature of 20°C, and (2) for load-losses, at the temperature of 75°C and 35 percent of nameplate load. (Source: Table 4–2 of NEMA Standard TP–1–2002, “Guide for Determining Energy Efficiency for Distribution Transformers.”)
|  |  |  |  |  |  |  |  |  |  |  |

#### Table T-4 Standards for Liquid-Immersed Distribution Transformers

Single phase | Three phase
kVA | Efficiency (%)¹ | kVA | Efficiency (%)¹
| Effective January 1, 2007 | Effective January 1, 2016 |  | Effective January 1, 2007 | Effective January 1, 2016
10 | 98.62 | 15 | 98.36 | 98.65
15 | 98.76 | 30 | 98.62 | 98.83
25 | 98.91 | 45 | 98.76 | 98.92
37.5 | 99.01 | 75 | 98.91 | 99.03
50 | 99.08 | 112.5 | 99.01 | 99.11
75 | 99.17 | 150 | 99.08 | 99.16
100 | 99.23 | 225 | 99.17 | 99.23
167 | 99.25 | 300 | 99.23 | 99.27
250 | 99.32 | 500 | 99.25 | 99.35
333 | 99.36 | 750 | 99.32 | 99.40
500 | 99.42 | 1000 | 99.36 | 99.43
667 | 99.46 | 1500 | 99.42 | 99.48
833 | 99.49 | 2000 | 99.46 | 99.51
|  | 2500 | 99.49 | 99.53
¹ Note: All efficiency values are at 50 percent of nameplate-rated load, determined when tested according to the test procedure in Section 1604(t).
|  |  |  |  |  |  |

#### Table T-5 Standards for Medium-Voltage Dry-Type Distribution Transformers Manufactured On or After January 1, 2010 and Before January 1, 2016

Single phase | Three phase
BIL kVA | 20‐45 kV Efficiency¹ (%) | 46‐95 kV Efficiency¹ (%) | ≥ 96 kV Efficiency¹ (%) | BIL kVA | 20‐45 kV Efficiency¹ (%) | 46‐95 kV Efficiency¹ (%) | ≥ 96 kV Efficiency¹ (%)
15 | 98.10 | 97.86 |  | 15 | 97.50 | 97.18 |
25 | 98.33 | 98.12 |  | 30 | 97.90 | 97.63 |
37.5 | 98.49 | 98.30 |  | 45 | 98.10 | 97.86 |
50 | 98.60 | 98.42 |  | 75 | 98.33 | 98.12 |
75 | 98.73 | 98.57 | 98.53 | 112.5 | 98.49 | 98.30 |
100 | 98.82 | 98.67 | 98.63 | 150 | 98.60 | 98.42 |
167 | 98.96 | 98.83 | 98.80 | 225 | 98.73 | 98.57 | 98.53
250 | 99.07 | 98.95 | 98.91 | 300 | 98.82 | 98.67 | 98.63
333 | 99.14 | 99.03 | 98.99 | 500 | 98.96 | 98.83 | 98.80
500 | 99.22 | 99.12 | 99.09 | 750 | 99.07 | 98.95 | 98.91
667 | 99.27 | 99.18 | 99.15 | 1000 | 99.14 | 99.03 | 98.99
833 | 99.31 | 99.23 | 99.20 | 1500 | 99.22 | 99.12 | 99.09
|  |  |  | 2000 | 99.27 | 99.18 | 99.15
|  |  |  | 2500 | 99.31 | 99.23 | 99.20
¹ All efficiency values are at 50 percent of nameplate rated load, determined when tested according to the test procedure in Section 1604(t).

#### Table T-6 Standards for Medium-Voltage Dry-Type Distribution Transformers
Manufactured On or After January 1, 2016

Single phase | Three phase
BIL kVA | 20‐45 kV Efficiency¹ (%) | 46‐95 kV Efficiency¹ (%) | ≥ 96 kV Efficiency¹ (%) | BIL kVA | 20‐45 kV Efficiency¹ (%) | 46‐95 kV Efficiency¹ (%) | ≥ 96 kV Efficiency¹ (%)
15 | 98.10 | 97.86 |  | 15 | 97.50 | 97.18 |
25 | 98.33 | 98.12 |  | 30 | 97.90 | 97.63 |
37.5 | 98.49 | 98.30 |  | 45 | 98.10 | 97.86 |
50 | 98.60 | 98.42 |  | 75 | 98.33 | 98.13 |
75 | 98.73 | 98.57 | 98.53 | 112.5 | 98.52 | 98.36 |
100 | 98.82 | 98.67 | 98.63 | 150 | 98.65 | 98.51 |
167 | 98.96 | 98.83 | 98.80 | 225 | 98.82 | 98.69 | 98.57
250 | 99.07 | 98.95 | 98.91 | 300 | 98.93 | 98.81 | 98.69
333 | 99.14 | 99.03 | 98.99 | 500 | 99.09 | 98.99 | 98.89
500 | 99.22 | 99.12 | 99.09 | 750 | 99.21 | 99.12 | 99.02
667 | 99.27 | 99.18 | 99.15 | 1000 | 99.28 | 99.20 | 99.11
833 | 99.31 | 99.23 | 99.20 | 1500 | 99.37 | 99.30 | 99.21
|  |  |  | 2000 | 99.43 | 99.36 | 99.28
|  |  |  | 2500 | 99.47 | 99.41 | 99.33
¹ All efficiency values are at 50 percent of nameplate rated load, determined when tested according to the test procedure in Section 1604(t).

#### Table U-1 Standards for Class A External Power Supplies That are Federally Regulated

Nameplate Output | Minimum Efficiency in Active Mode (Decimal equivalent of a Percentage)
< 1 watt | 0.5 * Nameplate Output
≥ 1 and ≤ 51 watts | 0.09*Ln(Nameplate Output) + 0.5
> 51 watts | 0.85
| Maximum Energy Consumption in No-Load Mode
≤ 250 watts | 0.5 watts
Where Ln (Nameplate Output) = Natural Logarithm of the nameplate output expressed in watts.

#### Table A-9 Standards for Wine Chillers

Appliance | Maximum Annual Energy Consumption (kWh)
Wine chillers with manual defrost | 13.7V + 267
Wine chillers with automatic defrost | 17.4V + 344
V = volume in ft³.

#### Table A-10 Standards for Freezers that are Consumer Products

Appliance | Maximum Annual Energy Consumption (kWh)
Upright Freezers with manual defrost | 7.55AV + 258.3
Upright Freezers with automatic defrost | 12.43AV + 326.1
Chest Freezers | 9.88AV + 143.7
AV = adjusted total volume, expressed in ft³, which is 1.73 x freezer volume (ft³).

#### Table A-12 Standards for Refrigerated Canned and Bottled Beverage Vending Machines

Appliance | Doors | Maximum Daily Energy Consumption (kWh)
January 1, 2006 | January 1, 2007
Refrigerated canned and bottled beverage vending machines when tested at 90° F ambient temperature except multi-package units | Not applicable | 0.55(8.66 + (0.009 × C)) | 0.55(8.66 + (0.009 × C))

#### Table C-7 Standards for Ground Water-Source and Ground-Source Heat Pumps

Appliance | Rating Condition | Minimum Standard
Ground water-source heat pumps (cooling) | 59°F entering water temperature | 16.2 EER
Ground water-source heat pumps (heating) | 50°F entering water temperature | 3.6 COP
Ground-source heat pumps (cooling) | 77°F entering brine temperature | 13.4 EER
Ground-source heat pumps (heating) | 32°F entering brine temperature | 3.1 COP

#### Table C-8 Standards for Evaporatively Cooled Computer Room Air Conditioners

Appliance | Cooling Capacity (Btu/hr) | Minimum EER (Btu/watt‐hour)
Air‐Cooled Effective January 1, 2006 | Water‐Cooled, Glycol‐Cooled, and Evaporatively‐Cooled Effective October 29, 2006
Computer room air conditioners | < 65,000 | 11.0 | 11.1
≥ 65,000 and < 135,000 | 10.4 | 10.5
≥ 135,000 and < 240,000 | 10.2 | 10.0

#### Table E-7 Standards for Boilers

Appliance | Output (Btu/hr) | Minimum AFUE % | Minimum Combustion Efficiency % * | Maximum Standby Loss (watts)
Gas steam boilers with 3-phase electrical supply | < 300,000 | 75 | — | —
All other boilers with 3-phase electrical supply | < 300,000 | 80 | — | —
Natural gas, non-packaged boilers | ≥ 300,000 | — | 80 | 147
LPG Non-packaged boilers | ≥ 300,000 | — | 80 | 352
Oil, non-packaged boilers | ≥ 300,000 | — | 83 | —
*At both maximum and minimum rated capacity, as provided and allowed by the controls.

#### Table E-8 Standards for Furnaces

Appliance | Application | Minimum Efficiency %
Central furnaces with 3-phase electrical supply < 225,000 Btu/hour | Mobile Home | 75 AFUE
All others | 78 AFUE or 80 Thermal Efficiency (at manufacturer’s option)

#### Table E-9 Standards for Duct Furnaces

Appliance | Fuel | Standards
Minimum Thermal Efficiency %¹ | Maximum Energy Consumption during standby (watts)
At maximum rated capacity | At minimum rated capacity
Duct furnaces | Natural gas | 80 | 75 | 10
Duct furnaces | LPG² | 80 | 75 | 147
¹ As provided and allowed by the controls. ² Designed expressly for use with LPG.

#### Table F-4 Standards for Small Water Heaters that are Not Federally-Regulated Consumer Products

Appliance | Energy Source | Input Rating | Rated Storage Volume (gallons) | Minimum Energy Factor¹
Storage water heaters | Gas | ≤ 75,000 Btu/hr | < 20 | 0.62 – (.0019 x V)
Storage water heaters | Gas | ≤ 75,000 Btu/hr | > 100 | 0.62 – (.0019 x V)
Storage water heaters | Oil | ≤ 105,000 Btu/hr | > 50 | 0.59 – (.0019 x V)
Storage water heaters | Electricity | ≤ 12 kW | > 120 | 0.93 – (.00132 x V)
Instantaneous Water Heaters | Gas | ≤ 50,000 Btu/hr | Any | 0.62 – (.0019 x V)
Instantaneous Water Heaters | Gas | ≤ 200,000 Btu/hr | ≥ 2 | 0.62 – (.0019 x V)
Instantaneous Water Heaters | Oil | ≤ 210,000 Btu/hr | Any | 0.59 – (.0019 x V)
Instantaneous Water Heaters | Electricity | ≤ 12 kW | Any | 0.93 – (.00132 x V)
¹ Volume (V) = rated storage volume in gallons.

#### Table H-2 Standards for Tub Spout Diverters

Appliance | Testing Conditions | Maximum Leakage Rate
Tub spout diverters | When new | 0.01 gpm
After 15,000 cycles of diverting | 0.05 gpm

#### Table K-9 Standards for State-Regulated Incandescent Reflector Lamps

Rated Lamp Wattage | Minimum Average Lamp Efficacy (LPW)
40-50 | 10.5
51-66 | 11.0
67-85 | 12.5
86-115 | 14.0
116-155 | 14.5
156-205 | 15.0

#### Table K-10 Standards for State-Regulated General Service Incandescent Lamps -Tier I

Rated Lumen Ranges | Maximum Rated Wattage | Minimum Rated Lifetime | Effective Date
1490-2600 Lumens | 72 watts | 1,000 Hours | Jan, 1, 2011
1050-1489 Lumens | 53 watts | 1,000 Hours | Jan 1, 2012
750-1049 Lumens | 43 watts | 1,000 Hours | Jan 1, 2013
310-749 Lumens | 29 watts | 1,000 Hours | Jan 1, 2013

#### Table K-11 Standards for State-Regulated General Service Lamps -Tier II

Lumen Ranges | Minimum Lamp Efficacy | Minimum Rated Lifetime | Effective Date
All | 45 lumens per watt | 1,000 Hours | Jan, 1, 2018

#### Table K-12 Standards for State-Regulated Modified
Spectrum General Service Incandescent Lamps -Tier I

Rated Lumen Ranges | Maximum Rated Wattage | Minimum Rated Lifetime | Effective Date
1118-1950 Lumens | 72 watts | 1,000 Hours | Jan 1, 2011
788-1117 Lumens | 53 watts | 1,000 Hours | Jan 1, 2012
563-787 Lumens | 43 watts | 1,000 Hours | Jan 1, 2013
232-562 Lumens | 29 watts | 1,000 Hours | Jan 1, 2013

#### Table L-1 Ultrasound Maximum Decibel Values

Mid-frequency of Sound Pressure Third-Octave Band (in kHz) | Maximum db Level within third-Octave Band(in dB reference 20 micropascals)
Less than 20 | 80
20 or more to less than 25 | 105
25 or more to less than 31.5 | 110
31.5 or more | 115

#### Table M-2 Standards for Traffic Signal Modules for Pedestrian
Control Sold or Offered for Sale in California

Type | at 25°C (77°F) | At 74°C (165.2°F)
Hand or ‘Don’t Walk’ sign or countdown. | 10 watts | 12 watts
Walking Person or ‘Walk’ sign | 9 watts | 12 watts

#### Table N-1 Standards for Under-Cabinet Luminaires

Lamp Length (inches) | Minimum Ballast Efficacy Factor (BEF) for one lamp | Minimum Ballast Efficacy Factor (BEF) for two lamps
≤29 | 4.70 | 2.80
>29 and ≤35 | 3.95 | 2.30
>35 and ≤41 | 3.40 | 1.90
>41 and ≤47 | 3.05 | 1.65
>47 | 2.80 | 1.45

#### Table N-2 Minimum Requirements for Portable LED Luminaires, and
Portable Luminaires with LED Light Engines with Integral Heat Sink

Criteria | Requirement
Light Output | ≥ 200 lumens (initial)
Minimum LED Luminaire Efficacy | 29 lumens/W
Minimum LED Light Engine Efficacy | 40 lumens/W
Color Correlated Temperature (CCT) | 2700 K through 5000 K
Minimum Color Rendering Index (CRI) | 75
Power Factor (for luminaires labeled or sold for residential use) | ≥ 0.70

#### Table U-2 Standards for State-Regulated External Power Supplies Effective January 1, 2007

for external power supplies used with laptop computers, mobile phones, printers, print
servers, canners, personal digital assistants (PDAs), and digital cameras, Effective July 1, 2007
for external power supplies used with wireline telephones and all other applications.

Nameplate Output | Minimum Efficiency in Active Mode
0 to < 1 watt | 0.49 * Nameplate Output
≥ 1 and ≤ 49 watts | 0.09 * Ln(Nameplate Output) + 0.49
> 49 watts | 0.84
| Maximum Energy Consumption in No-Load Mode
0 to <10 watts | 0.5 watts
≥ 10 to ≤ 250 watts | 0.75 watts
Where Ln (Nameplate Output) = Natural Logarithm of the nameplate output expressed in watts.

#### Table U-3 Standards for State-Regulated External Power Supplies
Effective July 1, 2008

Nameplate Output | Minimum Efficiency in Active Mode
<1 watt | 0.5 * Nameplate Output
≥ 1 and ≤ 51 watts | 0.09*Ln(Nameplate Output) + 0.5
> 51 watts | 0.85
| Maximum Energy Consumption in No-Load Mode
Any output | 0.5 watts
Where Ln (Nameplate Output) = Natural Logarithm of the nameplate output expressed in watts.

#### Table V-1 Standards for Consumer Audio and Video Equipment

Appliance Type | Effective Date | Maximum Power Usage (Watts)
Compact Audio Products | January 1, 2007 | 2 W in Audio standby-passive mode for those without a permanently illuminated clock display 4 W in Audio standby-passive mode for those with a permanently illuminated clock display
Digital Versatile Disc Players and Digital Versatile Disc Recorders | January 1, 2006 | 3 W in Video standby-passive mode

#### Table V-2 Standards for Televisions

Effective Date | Screen Size (area A in square inches) | Maximum TV Standby-passive Mode Power Usage (watts) | Maximum On Mode Power Usage (P in Watts) | Minimum Power Factor for (P ≥ 100W)
January 1, 2006 | All | 3 W | No standard | No standard
January 1, 2011* | A < 1400 | 1 W | P ≤ 0.20 x A + 32 | 0.9
January 1, 2013 | A < 1400 | 1 W | P ≤ 0.12 x A + 25 | 0.9

#### Table W-1 Standards for Large Battery Charger Systems

Performance Parameter | Standard
Charge Return Factor (CRF) | 100 percent, 80 percent Depth of discharge | CRF≤ 1.10
40 percent Depth of discharge | CRF ≤ 1.15
Power Conversion Efficiency | Greater than or equal to: 89 percent
Power Factor | Greater than or equal to: 0.90
Maintenance Mode Power (Eb = battery capacity of tested battery) | Less than or equal to: 10 + 0.0012Eb W
No Battery Mode Power | Less than or equal to: 10 W

#### Table W-2 Standards for Small Battery Charger Systems

Performance Parameter | Standard
Maximum 24 hour charge and maintenance energy (Wh) (Eb = capacity of all batteries in ports and N = number of charger ports) | For Eb of 2.5 Wh or less: 16 × N
For Eb greater than 2.5 Wh and less than or equal to 100 Wh: 12 x N +1.6Eb
For Eb greater than 100 Wh and less than or equal to 1000 Wh: 22 x N+1.5Eb
For Eb greater than 1000 Wh: 36.4 x N +1.486Eb
Maintenance Mode Power and No Battery Mode Power (W) (Eb = capacity of all batteries in ports and N = number of charger ports) | The sum of maintenance mode power and no battery mode power must be less than or equal to: 1x N+0.0021xEb