## Appendix B

Applicable Tables and Language from Standards and RACM

Appendix B is a collection of common used tables and language that are referenced in the Residential Compliance Manual which includes excerpts from the 2013 Building Energy Efficiency Standards for Residential and Nonresidential Buildings and the Appliance Efficiency Regulations.

#### FIGURE 100.1-A—CALIFORNIA CLIMATE ZONES

#### TABLE 100.0-A APPLICATION OF STANDARDS

Occupancies | Application | Mandatory | Prescriptive | Performance | Additions/Alterations
General Provisions | 100.0, 100.1, 100.2, 110.0, 110.10
Nonresidential, High-Rise Residential, And Hotels/Motels | General | 140.0 | 140.2 | 140.1 | 141.0
Envelope (conditioned) | 110.6, 110.7, 110.8, 120.7 | 140.3
Envelope (unconditioned process spaces) | N.A. | 140.3(c)
HVAC (conditioned) | 110.2, 110.5, 120.0-120.5, 120.8 | 140.4
Water Heating | 110.3, 120.3, 120.8 | 140.5
Indoor Lighting (conditioned, process spaces) | 110.9, 120.8, 130.0, 130.1, 130.4 | 140.3(c), 140.6
Indoor Lighting (unconditioned and parking garages) | 110.9, 120.8, 130.0, 130.1, 130.4 | 140.3(c), 140.6 | N.A.
Outdoor Lighting | 110.9, 130.0, 130.2, 130.4 | 140.7
Building Electrical Power | 130.5 | N.A.
Pool and Spa Systems | 110.4, 150.0(p) | N. A. | N. A.
Solar Ready Buildings | 110.10 | N.A. | N.A.
Covered Processes1 | Envelope, Ventilation, Process Loads | 110.2, 120.6, 120.8 | 140.9 | 140.1 | 120.6, 140.9
Signs | Indoor and Outdoor | 130.0, 130.3 | 140.8 | N.A. | 141.0
Low-Rise Residential | General | 150.0 | 150.1 (a, c) | 150.1 (a, b) | 150.2
Envelope (conditioned) | 110.6, 110.7, 110.8, 150.0(a-e, g, l)
HVAC (conditioned) | 110.2, 110.5, 150.0(h, i, m, o)
Water Heating | 110.3, 150.0(j, n)
Indoor Lighting (conditioned, unconditioned and parking garages) | 110.9, 130.0, 150.0(k)
Outdoor Lighting | 110.9, 130.0, 150.0(k)
Pool and Spa Systems | 110.4, 150.0(p) | N. A. | N.A. | N.A.
Solar Ready Buildings | 110.10 | N. A. | N.A. | N.A.
1 Nonresidential, high-rise and hotel/motel buildings that contain covered processes may conform to the applicable requirements of both occupancy types 'listed in this table.

#### TABLE 110.2-A ELECTRICALLY OPERATED UNITARY AIR CONDITIONERS AND CONDENSING UNITS – MINIMUM EFFICIENCY REQUIREMENTS

Equipment Type | Size Category | Efficiency a | Test Procedurec
Before 1/1/2015 | After 1/1/2015 |
Air conditioners, air cooled both split system and single package | ≥ 65,000 Btu/h and < 135,000 Btu/h | 11.2 EERb 11.4 IEERb | Applicable minimum efficiency values as determined by Title 20 California Code of Regulations Section 1605.1 | ANSI/AHRI 340/360
≥ 135,000 Btu/h and < 240,000 Btu/h | 11.0 EERb 11.2 IEERb | ANSI/AHRI 340/360
≥ 240,000 Btu/h and < 760,000 Btu/h | 10.0 EERb 10.1 IEERb
≥ 760,000 Btu/h | 9.7 EERb 9.8 IEERb |
Air conditioners, water cooled | ≥ 65,000 Btu/h and < 135,000 Btu/h | 12.1 EERb 12.3 IEERb | ANSI/AHRI 340/360
≥135,000 Btu/h and < 240,000 Btu/h | 12.5 EERb 12.5 IEERb | ANSI/AHRI 340/360
≥240,000 Btu/h and < 760,000 Btu/h | 12.4 EERb 12.6 IEERb | ANSI/AHRI 340/360
≥ 760,000 Btu/h | 12.2 EERb 12.4 IEERb | NSI/AHRI 340/360
Air conditioners, evaporatively cooled | ≥65,000 Btu/h and < 135,000 Btu/h | 12.1 EERb 12.3 IEERb | ANSI/AHRI 340/360
≥ 135,000 Btu/h and < 240,000 Btu/h | 12.0 EERb 12.2 IEERb | ANSI/AHRI 340/360
≥240,000 Btu/h and < 760,000 Btu/h | 11.9 EERb 12.1 IEERb | ANSI/AHRI 340/360
≥ 760,000 Btu/h | 11.7 EERb 11.9 IEERb | ANSI/AHRI 340/360
Condensing units, air cooled | ≥ 135,000 Btu/h | 10.5 EER 11.8 IEER | ANSI/AHRI 365
Condensing units, water cooled | ≥ 135,000 Btu/h | 13.5 EER 14.0 IEER
Condensing units, evaporatively cooled | ≥ 135,000 Btu/h | 13.5 EER 14.0 IEER
a. IEERs are only applicable to equipment with capacity control as per ANSI/AHRI 340/360 test procedures b. Deduct 0.2 from the required EERs and IEERs for units with a heating section other than electric resistance heat. c. Applicable test procedure and reference year are provided under the definitions.

Standards Tables 110.2-B

#### TABLE 110.2-B UNITARY AND APPLIED HEAT PUMPS, MINIMUM EFFICIENCY REQUIREMENTS

Equipment Type | Size Category | Subcategory or Rating Condition | Efficiency a | Test Procedure c
Air Cooled (Cooling Mode) | ≥ 65,000 Btu/h and < 135,000 Btu/h | Split system and single package | 11.0 EERb 11.2 IEERb | ANSI/AHRI 340/360
≥ 135,000 Btu/h and < 240,000 Btu/h | 10.6 EERb 10.7 IEERb
≥ 240,000 Btu/h | 9.5 EERb 9.6 IEERb
Water source (cooling mode) | ≥ 65,000 Btu/h and < 135,000 Btu/h | 86ºF entering water | 12.0 EER | ISO-13256-1
Groundwater source (cooling mode) | < 135,000 Btu/h | 59ºF entering water | 16.2 EER | ISO-13256-1
Ground source (cooling mode) | < 135,000 Btu/h | 77ºF entering water | 13.4 EER | ISO-13256-1
Water source water-to-water (cooling mode) | < 135,000 Btu/h | 86ºF entering water | 10.6 EER | ISO-13256-2
Groundwater source water-to-water (cooling mode) | < 135,000 Btu/h | 59ºF entering water | 16.3 EER | ISO-13256-1
Ground source brine-to-water (cooling mode) | < 135,000 Btu/h | 77ºF entering water | 12.1 EER | ISO-13256-2
Air Cooled (Heating Mode) Split system and single package | ≥ 65,000 Btu/h and < 135,000 Btu/h (cooling capacity) | 47° F db/43° F wb outdoor air | 3.3 COP | ANSI/AHRI 340/360
17° F db/15° F wb outdoor air | 2.25 COP
≥ 135,000 Btu/h (cooling capacity) | 47° F db/43° F wb outdoor air | 3.2 COP
| 17° F db/15° F wb outdoor air | 2.05 COP
Water source (heating mode) | < 135,000 Btu/h (cooling capacity) | 68ºF entering water | 4.2 COP | ISO-13256-1
Groundwater source (heating mode) | < 135,000 Btu/h (cooling capacity) | 50ºF entering water | 3.6 COP | ISO-13256-1
Ground source (heating mode) | < 135,000 Btu/h (cooling capacity) | 32ºF entering water | 3.1 COP | ISO-13256-1
Water source water-to-water (heating mode) | < 135,000 Btu/h (cooling capacity) | 68ºF entering water | 3.7 COP | ISO-13256-2
Groundwater source water-to-water (heating mode) | < 135,000 Btu/h (cooling capacity) | 50ºF entering water | 3.1 COP | ISO-13256-2
Ground source brine-to-water (heating mode) | < 135,000 Btu/h (cooling capacity) | 32ºF entering water | 2.5 COP | ISO-13256-2
a IEERs are only applicable to equipment with capacity control as per ANSI/AHRI 340/360 test procedures. b Deduct 0.2 from the required EERs and IEERs for units with a heating section other than electric resistance heat. c Applicable test procedure and reference year are provided under the definitions.

Standards Tables 110.6-A and 110.6-B

#### TABLE 110.6-A DEFAULT FENESTRATION PRODUCT U-FACTORS

FRAME | PRODUCT TYPE | SINGLE PANE 3, 4 U-FACTOR | DOUBLE PANE 1, 3, 4 U-FACTOR | GLASS BLOCK 2,3 U-FACTOR
Metal | Operable | 1.28 | 0.79 | 0.87
Fixed | 1.19 | 0.71 | 0.72
Greenhouse/garden window | 2.26 | 1.40 | N.A.
Doors | 1.25 | 0.77 | N.A.
Skylight | 1.98 | 1.30 | N.A.
Metal, Thermal Break | Operable | N.A. | 0.66 | N.A.
Fixed | N.A. | 0.55 | N.A.
Greenhouse/garden window | N.A. | 1.12 | N.A.
Doors | N.A. | 0.59 | N.A.
Skylight | N.A. | 1.11 | N.A.
Nonmetal | Operable | 0.99 | 0.58 | 0.60
Fixed | 1.04 | 0.55 | 0.57
Doors | 0.99 | 0.53 | N.A.
Greenhouse/garden windows | 1.94 | 1.06 | N.A.
Skylight | 1.47 | 0.84 | N.A.
For all dual-glazed fenestration products, adjust the listed U-factors as follows: Add 0.05 for products with dividers between panes if spacer is less than 7/16 inch wide. Add 0.05 to any product with true divided lite (dividers through the panes). Translucent or transparent panels shall use glass block values when not rated by NFRC 100. Visible Transmittance (VT) shall be calculated by using Reference Nonresidential Appendix NA6. Windows with window film applied that is not rated by NFRC 100 shall use the default values from this table.

#### TABLE 110.6-B DEFAULT SOLAR HEAT GAIN COEFFICIENT (SHGC)

FRAME TYPE | PRODUCT | GLAZING | FENESTRATION PRODUCT SHGC
Single Pane2,3 SHGC | Double Pane2,3 SHGC | Glass Block1,2 SHGC
Metal | Operable | Clear | 0.80 | 0.70 | 0.70
Fixed | Clear | 0.83 | 0.73 | 0.73
Operable | Tinted | 0.67 | 0.59 | N.A.
Fixed | Tinted | 0.68 | 0.60 | N.A.
Metal, Thermal Break | Operable | Clear | N.A. | 0.63 | N.A.
Fixed | Clear | N.A. | 0.69 | N.A.
Operable | Tinted | N.A. | 0.53 | N.A.
Fixed | Tinted | N.A. | 0.57 | N.A.
Nonmetal | Operable | Clear | 0.74 | 0.65 | 0.70
Fixed | Clear | 0.76 | 0.67 | 0.67
Operable | Tinted | 0.60 | 0.53 | N.A.
Fixed | Tinted | 0.63 | 0.55 | N.A.
Translucent or transparent panels shall use glass block values when not rated by NFRC 200. Visible Transmittance (VT) shall be calculated by using Reference Nonresidential Appendix NA6. Windows with window film applied that is not rated by NFRC 200 shall use the default values from this table.

Standards Tables 150.1-A

#### STANDARDS TABLE 150.1-A COMPONENT PACKAGE A

| Climate Zone
1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Building Envelope | Insulation1 | Roofs /Ceilings U / R-Value | U 0.025 /R38 | U 0.031/R 30 | U 0.025 /R 38
Walls | Above Grade | 2x4 Framed2 | U 0.065 /R 15+4/ or R 13+5
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Mass Wall Interior3 | U 0.070 /R 13 | U 0.059 /R 17
Mass Wall Exterior3 | U 0.125 /R 8.0 | U 0.070 /R 13
Below Grade | Below Grade Interior3 | U 0.070 /R 13 | U 0.066 /R 15
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Below Grade Exterior3 | U 0.200 /R 5.0 | U 0.100 /R 10 | U 0.053 /R 19
Floors | Slab Perimeter | NR | U 0.58 /R 7
Raised | U 0.037 /R 19
|  |  |  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Concrete Raised | U 0.092 R 8.0 | U 0.269 /R 0.0 | U 0.092 /R 8.0 | U 0.138 /R 4.0 | U 0.092 /R 8.0 | U 0.092 /R 8.0 | U 0.138 /R 4.0 | U 0.092 /R 8.0
Radiant Barrier | NR | REQ | NR
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Building Envelope | Roofing Products | Low- sloped |  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Aged Solar Reflectance | NR | 0.63 | NR | 0.63 | NR
Thermal Emittance | NR | 0.75 | NR | 0.75 | NR
Steep Sloped | Aged Solar Reflec- tance | NR | 0.20 | NR
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Thermal Emittance | NR | 0. 75 | NR
Fenestration | Maximum U-factor4 | 0.32
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Maximum SHGC5 | NR | 0.25 | NR | 0.25 | NR | 0.25
Maximum Total Area | 20%
Maximum West Facing Area | NR | 5% | NR | 5% | NR | 5%
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

#### TABLE 150.1-A COMPONENT PACKAGE A (continuation)

|  |  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
HVAC SYSTEM | Space Heating | Electric Resistance Allowed | Not Allowed
If gas, AFUE | Minimum
If Heat Pump, HSPF6 | Minimum
Space Cooling | SEER | Minimum
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Refrigerant Charge Verification or Charge Indicator Display | NR | REQ | NR | REQ | NR
Whole House Fan7 | NR | REQ | NR | NR
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Central System Air Handler | Central Fan Integrated Ventilation Systems Fan Efficacy | REQ
Ducts | Duct Insulation | R-6 | R-8 | R-6 | R-8 | R-8 | R-8
|  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
Water Heating | All Buildings | System Shall meet Section 150.1(c)8
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Footnote requirements to TABLE 150.1-A.

1. The U-factors/R-values shown for ceiling, wall and raised floor insulation are for wood-frame construction with insulation installed between the framing members. For alternative construction assemblies, see Section 150.1(c)1A, B and C.

2. U-factors can be met by cavity insulation alone or with continuous insulation alone, or with both cavity and continuous insulation that results in a U-factor equal to or less than the U-factor shown. “R-15+4” means R-15 cavity insulation plus R-4 continuous insulation. Any combination of cavity insulation and/or continuous insulation that results in a U-factor equal to or less than 0.065 is allowed, such as R-13+5.

3 Mass wall has a thermal heat capacity greater than or equal to 7.0 Btu/h-ft2. Below grade “interior” denotes insulation installed on the inside surface of the wall. Below grade “exterior” denotes insulation installed on the outside surface of the wall.

4. The installed fenestration products shall meet the requirements of Section 150.1(c)3.

5. The installed fenestration products shall meet the requirements of Section 150.1(c)4.

6. HSPF means "heating seasonal performance factor."

7. When whole house fans are required (REQ), only those whole house fans that are listed in the Appliance Efficiency Directory may be installed. Compliance requires installation of one or more WHFs whose total airflow CFM is capable of meeting or exceeding a minimum 2 cfm/square foot of conditioned floor area per Section 150.1(c)12.

8. A supplemental heating unit may be installed in a space served directly or indirectly by a primary heating system, provided that the unit thermal capacity does not exceed 2 kilowatts or 7,000 Btu/hr and is controlled by a time-limiting device not exceeding 30 minutes.

Standards Tables 150.2-A Aged Solar Reflectance Insulation Trade off Table

#### Table 150.2-A Aged Solar Reflectance Insulation Trade off Table

Aged Solar Reflectance | Roof Deck Insulation R-value | Aged Solar Reflectance | Roof Deck Insulation R-value
0.62-0.60 | 2 | 0.44-0.40 | 12
0.59-0.55 | 4 | 0.39-0.35 | 16
0.54-0.50 | 6 | 0.34-0.30 | 20
0.49-0.45 | 8 | 0.29-0.25 | 24

Residential Table – Vintage Table Values

#### TABLE R3-50 – DEFAULT ASSUMPTIONS FOR EXISTING BUILDINGS – VINTAGE TABLE VALUES

Default Assumptions for Year Built (Vintage)
Conservation Measure | Before 1978 | 1978 to 1983 | 1984 to 1991 | 1992 to 1998 | 1999 -2000 | 2001-2003 | 2004-2005 | 2006 and 2012 | 2013 and Later
INSULATION U-FACTOR |  |  |  |  |  |  |  |  |
Roof/Ceiling |  | 0.079 | 0.049 | 0.049 | 0.049 | 0.049 | 0.049 | 0.049 | 0.049 |
Wall |  | 0.356 | 0.110 | 0.110 | 0.102 | 0.102 | 0.102 | 0.102 | 0.102 |
Raised Floor –Crawl Space | 0.099 | 0.099 | 0.099 | 0.046 | 0.046 | 0.046 | 0.046 | 0.046 |
Cool Roof | 0.10 | 0.10 | 0.10 | 0.10 | 0.10 | 0.10 | 0.10 | Pres Pkg. |
Radiant Barrier | None | None | None | None | None | None | Pres Pkg. | Pres Pkg. |
Raised Floor-No Crawl Space | 0.238 | 0.238 | 0.238 | 0.064 | 0.064 | 0.064 | 0.064 | 0.064 |
Slab Edge | F-factor | 0.73 | 0.73 | 0.73 | 0.73 | 0.73 | 0.73 | 0.73 | 0.73 |
Ducts |  | R-2.1 | R-2.1 | R-2.1 | R-4.2 | R-4.2 | R-4.2 | R-4.2 | Pres Pkg. |
LEAKAGE |  |  |  |  |  |  |  |  |
Building (SLA) | 4.9 | 4.9 | 4.9 | 4.9 | 4.9 | 4.9 | 4.9 | 4.9 |
Duct Leakage Factor (See Table 4-13) | 0.86 | 0.86 | 0.86 | 0.86 | 0.86 | 0.89 | 0.89 | 0.89 |
FENESTRATION
U-factor | Use Standards Table 110.6-A, §110.6 for all Vintages |
SHGC | Use Standards Table 110.6-B, §110.6 for all Vintages |
Shading Dev. | Use Table R3-27 and R3-28 for all Vintages in the Residential ACM Manual – Performance Approach |
SPACE HEATING EFFICIENCY
Gas Furnace (Central) AFUE | 0.75 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 |
Gas Heater (Room) AFUE | 0.65 | 0.65 | 0.65 | 0.65 | 0.65 | 0.65 | 0.65 | 0.65 |
Hydronic/Comb Hydronic | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 | 0.78 |
Heat Pump | HSPF | 5.6 | 5.6 | 6.6 | 6.6 | 6.8 | 6.8 | 6.8 | 7.4 |
Electric Resistance HSPF | 3.413 | 3.413 | 3.413 | 3.413 | 3.413 | 3.413 | 3.413 | 3.413 |
Electric Resistance Radiant HSPF | 3.55 | 3.55 | 3.55 | 3.55 | 3.55 | 3.55 | 3.55 | 3.55 |
SPACE COOLING EFFICIENCY |  |  |  |  |  |  |  |  |
All Types, | SEER | 8.0 | 8.0 | 8.9 | 9.7 | 9.7 | 9.7 | 9.7 | 13.0 |
WATER HEATING |  |  |  |  |  |  |  |  |
Energy Factor | 0.525 | 0.525 | 0.525 | 0.525 | 0.575 | 0.575 | 0.575 | 0.575 |
|  |  |  |  |  |  |  |  |  |  |  |  |

Appliance Efficiency Standards from Section 1605.1

#### Table B-2Standards for Room Air Conditioners and Room Air-Conditioning Heat Pumps

Appliance | Louvered Sides | Cooling Capacity (Btu/hr) | Minimum EER
Room Air Conditioner | Yes | < 6,000 | 9.7
Room Air Conditioner | Yes | ≥ 6,000 – 7,999 | 9.7
Room Air Conditioner | Yes | ≥ 8,000 – 13,999 | 9.8
Room Air Conditioner | Yes | ≥ 14,000 – 19,999 | 9.7
Room Air Conditioner | Yes | ≥ 20,000 | 8.5
Room Air Conditioner | No | < 6,000 | 9.0
Room Air Conditioner | No | ≥ 6,000 – 7,999 | 9.0
Room Air Conditioner | No | ≥ 8,000 – 19,999 | 8.5
Room Air Conditioner | No | ≥ 20,000 | 8.5
Room Air Conditioning Heat Pump | Yes | < 20,000 | 9.0
Room Air Conditioning Heat Pump | Yes | ≥ 20,000 | 8.5
Room Air Conditioning Heat Pump | No | < 14,000 | 8.5
Room Air Conditioning Heat Pump | No | ≥ 14,000 | 8.0
Casement-Only Room Air Conditioner | Either | Any | 8.7
Casement-Slider Room Air Conditioner | Either | Any | 9.5

#### Table B-3 Standards for Packaged Terminal Air Conditioners and Packaged Terminal Heat Pumps

Appliance | Mode | Cooling Capacity (Btu/hr) | Minimum EER or COP
Packaged terminal air conditioners and packaged terminal heat pumps | Cooling | ≤ 7,000 | 8.88 EER
> 7,000 and < 15,000 | 10.0 − (0.00016 x Cap.) EER
≥ 15,000 | 7.6 EER
Packaged terminal heat pumps | Heating | Any | 1.3 + [0.16 (10.0 – 0.00016 x Cap.)] COP
Cap. = cooling capacity (Btu/hr)

#### Table C-3 Standards for Air-Cooled Air Conditioners and Air-Source Heat Pumps Subject to EPAct
(Standards Effective January 1, 2010 do not apply To Single Package Vertical Air Conditioners)

Appliance | Cooling Capacity (Btu/hr) | System Type | Minimum Efficiency
Effective January 1, 1994¹ or January 1, 1995² | Effective June 15, 2008 | Effective January 1, 2010
Air Conditioners | Heat Pumps
Air-cooled unitary air conditioners and heat pumps (cooling mode) | < 65,000 * | Split system | 10.0 SEER¹ | 13.0 SEER |  |
< 65,000 * | Single package | 9.7 SEER¹ | 13.0 SEER |  |
≥ 65,000 and < 135,000 | All | 8.9 EER¹ |  | 11.2 EER³ 11.0 EER4 | 11.0 EER³ 10.8 EER4
≥ 135,000 and < 240,000 | All | 8.5 EER² |  | 11.0 EER³ 10.8 EER4 | 10.6 EER³ 10.4 EER4
≥ 240,000 and < 760,000 | All |  |  | 10.0 EER³ 9.8 EER4 | 9.5 EER³ 9.3 EER4
Air-cooled unitary air-conditioning heat pumps (heating mode) | < 65,000 * | Split system | 6.8 HSPF¹ | 7.7 HSPF |
< 65,000 * | Single package | 6.6 HSPF¹ | 7.7 HSPF |
≥ 65,000 and < 135,000 | All | 3.0 COP¹ |  | 3.3 COP
≥ 135,000 and < 240,000 | All | 2.9 COP² |  | 3.2 COP
≥ 240,000 and < 760,000 | All |  |  | 3.2 COP
* Three phase models only. ³ Applies to equipment that has electric resistance heat or no heating. 4 Applies to equipment with all other heating-system types that are integrated into the unitary equipment.

#### Table C-4Standards for Evaporatively-Cooled Air Conditioners

Appliance | Cooling Capacity (Btu per hour) | Minimum EER
Effective October 29, 2003 | Effective October 29, 2004
Evaporatively-cooled air conditioners | < 65,000 | 12.1 | 12.1
≥ 65,000 and < 135,000 | 11.5¹ | 11.5¹
≥ 135,000 < 240,000 | 9.6 | 11.0
¹ Deduct 0.2 from the required EER for units with heating sections other than electric resistance heat.

#### Table C-6Standards for Single Package Vertical Air Conditioners and Single Package Vertical Heat PumpsManufactured on or After January 1, 2010

Appliance | Cooling Capacity (BTU/hr) | System Type | Minimum Efficiency
Cooling Mode | Heating Mode
Single package vertical air conditioners | < 65,000 | Single-phase | 9.0 EER | N/A
< 65,000 | 3-phase | 9.0 EER | N/A
≥ 65,000 and < 135,000 | All | 8.9 EER | N/A
≥ 135,000 and < 240,000 | All | 8.6 EER | N/A
Single package vertical heat pumps | < 65,000 | Single-phase | 9.0 EER | 3.0 COP
< 65,000 | 3-phase | 9.0 EER | 3.0 COP
≥ 65,000 and < 135,000 | All | 8.9 EER | 3.0 COP
≥ 135,000 and < 240,000 | All | 8.6 EER | 2.9 COP

#### Table E-2 Standards for Gas Wall Furnaces, Floor Furnaces, and Room Heaters

Appliance | Design Type | Capacity (Btu per hour) | Minimum AFUE (%)
Wall furnace | Fan | ≤ 42,000 | 73
Wall furnace | Fan | > 42,000 | 74
Wall furnace | Gravity | ≤ 10,000 | 59
Wall furnace | Gravity | > 10,000 ≤ 12,000 | 60
Wall furnace | Gravity | > 12,000 ≤ 15,000 | 61
Wall furnace | Gravity | > 15,000 ≤ 19,000 | 62
Wall furnace | Gravity | > 19,000 ≤ 27,000 | 63
Wall furnace | Gravity | > 27,000 ≤ 46,000 | 64
Wall furnace | Gravity | > 46,000 | 65
Floor furnace | All | ≤ 37,000 | 56
Floor furnace | All | > 37,000 | 57
Room heater | All | ≤ 18,000 | 57
Room heater | All | > 18,000 and ≤ 20,000 | 58
Room heater | All | > 20,000 and ≤ 27,000 | 63
Room heater | All | > 27,000 and ≤ 46,000 | 64
Room heater | All | > 46,000 | 65

#### Table E-3Standards for Gas- and Oil-Fired Central Boilers and Electric Residential Boilers

Appliance | Rated Input (Btu/hr) | Minimum Efficiency (%)
AFUE | Combustion Efficiency at Maximum Rated Capacity Effective January 1, 1994
Effective January 1, 1992 | Effective September 1, 2012
Gas steam boilers with single phase electrical supply | < 300,000 | 75 | 80 ¹ | —
Gas hot water boilers with single phase electrical supply | < 300,000 | 80 | 82 ¹,² | —
Oil steam boilers with single phase electrical supply | < 300,000 | — | 82 | —
Oil hot water boilers with single phase electrical supply | < 300,000 | — | 84 ² | —
Electric steam residential boilers |  | — | NONE | —
Electric hot water residential boilers |  | — | NONE ² | —
All other boilers with single phase electrical supply | < 300,000 | 80 | — | —
Gas packaged boilers | ≥ 300,000 | — | — | 80
Oil packaged boilers | ≥ 300,000 | — | — | 83
¹ No constant burning pilot light design standard effective September 1, 2012. ² Automatic means for adjusting temperature design standard effective September 1, 2012.

#### Table F-3
Standards for Large Water Heaters Effective October 29, 2003

Appliance | Input to Volume Ratio | Size (Volume) | Minimum Thermal Efficiency (%) | Maximum Standby Loss¹,²
Gas storage water heaters | < 4,000 Btu/hr/gal | any | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Gas instantaneous water heaters | ≥ 4,000 Btu/hr/gal | < 10 gal | 80 | –
≥ 10 gal | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Gas hot water supply boilers | ≥ 4,000 Btu/hr/gal | < 10 gal | 80 | –
≥ 10 gal | 80 | Q/800 + 110(Vr)1/2 Btu/hr
Oil storage water heaters | < 4,000 Btu/hr/gal | any | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Oil instantaneous water heaters | ≥ 4,000 Btu/hr/gal | < 10 gal | 80 | –
≥ 10 gal | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Oil hot water supply boilers | ≥ 4,000 Btu/hr/gal | < 10 gal | 80 | –
≥ 10 gal | 78 | Q/800 + 110(Vr)1/2 Btu/hr
Electric storage water heaters | < 4,000 Btu/hr/gal | any | – | 0.3 + 27/Vm %/hr
¹ Standby loss is based on a 70° F temperature difference between stored water and ambient requirements. In the standby loss equations, Vr is the rated volume in gallons, Vm is the measured volume in gallons, and Q is the nameplate input rate in Btu/hr. ² Water heaters and hot water supply boilers having more than 140 gallons of storage capacity are not required to meet the standby loss requirement if the tank surface is thermally insulated to R-12.5, if a standing pilot light is not installed, and for gas- or oil-fired storage water heaters, there is a flue damper or fan-assisted combustion.

#### Table F-4
Standards for Small Federally-Regulated Water Heaters

Appliance | Minimum Energy Factor
Effective April 15, 1991 | Effective January 20, 2004
Gas-fired storage-type water heaters | 0.62 – (.0019 x V) | 0.67 – (.0019 x V)
Oil-fired water heaters (storage and instantaneous) | 0.59 – (.0019 x V) | 0.59 – (.0019 x V)
Electric storage water heaters (excluding tabletop water heaters) | 0.93 – (.00132 x V) | 0.97 – (.00132 x V)
Electric tabletop water heaters | 0.93 – (.00132 x V) | 0.93 – (.00132 x V)
Gas-fired instantaneous water heaters | 0.62 – (.0019 x V) | 0.62 – (.0019 x V)
Electric instantaneous water heaters (excluding tabletop water heaters) | 0.93 – (.00132 x V) | 0.93 – (.00132 x V)
Heat pump water heaters | 0.93 – (.00132 x V) | 0.97 – (.00132 x V)
V = rated volume in gallons.