## JA8.6 Data Reporting

The following test data shall be submitted to the California Energy Commission in the format specified in Table JA-8. The entity submitting the filing shall keep all test data and documentation required for compliance for at least two years from the date of certification and shall provide copies of this documentation to the Energy Commission within 10 days of written request received from the Energy Commission.

#### TABLE JA-8. DATA TO BE RECORDED AND SUBMITTED TO THE CALIFORNIA ENERGY COMMISSION

Required Information | Permissible Answers | Compliance Threshold
Manufacturer, Model number, Description |  |
Light Source Type | LED, OLED, Fluorescent, HID, Incandescent, Other |
Product type | Omnidirectional lamp, Directional lamp, Decorative lamp, LED light engine, inseparable SSL luminaire, other |
Lab accredited by NVLAP or accreditation body operating in accordance with ISO/IEC 17011? | Yes/No | Yes
Initial Efficacy | Value (lumens/Watt) | ≥ 45 lumens/Watt
Start time | Value (seconds) | ≤ 0.5 sec
Correlated Color Temperature (CCT) | Number Kelvin | For inseparable SSL luminaires, LED light engines and GU24 LED lamps, ≤4000 Kelvin. For all other sources,≤ 3000 Kelvin.
Duv | Number Duv | ≥-0.0033 and ≤ +0.0033
Color Rendering Index (CRI) | 0-100 | ≥ 90
Power Factor at Full Rated Power | 0 – 1 Fraction | ≥ 0.90
Color Rendering R9 (red) | 0-100 or below 0 | ≥ 50
Ambient or elevated temperature test for rated life, lumen maintenance, and survival rate | Ambient or Elevated | “Ambient” allowed only for omnidirectional lamps <10W, and decorative lamps, or labeled “not for use in enclosed fixtures”, lamps and light engines that are labeled “not for use in recessed fixtures” and “inseparable SSL luminaires”. All others must report “Elevated”.
6,000 hour lumen maintenance | Value (percent), N/A | ≥ 86.7% or NA for integral luminaires providing TM-21 L70 projections based on light source LM80 data
LM-80 and TM-21 Projected Time to L70 | Value (hours), N/A | ≥ 25,000 hours, or N/A for light sources providing 6,000 hour lumen maintenance testing
Rated life | Value (hours) | ≥ 15,000 hours
6,000 hour survival rate | Value (percent) | ≥ 90% or NA for integral luminaires whose lumen maintenance/rated life is evaluated using light source LM-80 data.
Minimum dimming level | Value (percent) | ≤ 10%
Dimming control compatibility | Forward Phase cut control, reverse phase cut, powerline carrier, digital, 0-10 VDC, other. | At least one type must be listed
NEMA SSL 7A compatible? | Yes/No | If compatible with forward phase cut dimmer control, “Yes”. If not, “No”.
Flicker:
See JA10 Table 10-1 for flicker data requirements and permissible answers |  | <30% for frequencies of 200 Hz or below, at 100% and 20% light output
Audible Noise
100% light output: Audible Noise | Value (dBA) | ≤ 24 dBA
20% light output: Audible Noise | Value (dBA) | ≤ 24 dBA
Marking
Marked in accordance with JA8.5 | Yes/No | Yes. “No” allowed only for lamps and LED light engines with diameter less than 1.0” and decorative lamps with a diameter less than 2.0”