## 10-102 – DEFINITIONS

In this article the following definitions apply:

'ACCEPTANCE REQUIREMENTS are "'acceptance requirements for code compliance" as defined in Section 100.1(b) of Part 6.

'ACCEPTANCE TEST TECHNICIAN is a Field Technician as defined in Section 10-102 who is certified by an authorized 'Acceptance Test Technician Certification Provider pursuant to the requirements of Sections 10-103.1 or 10-103.2.

'Lighting Controls 'Acceptance Test Technician is a professional certified by an authorized 'Lighting Controls 'Acceptance Test Technician Certification Provider to perform nonresidential lighting controls 'acceptance tests and complete the documentation required for nonresidential 'lighting controls acceptance tests as required by the ’Building Energy Efficiency Standards.

'Mechanical 'Acceptance Test Technician is a professional certified by an authorized 'Mechanical 'Acceptance Test Technician Certification Provider to perform nonresidential 'mechanical acceptance tests and complete the documentation required for nonresidential mechanical acceptance tests as required by the Building’ Energy Efficiency Standards.

'ACCEPTANCE TEST EMPLOYER is a person or entity who employs an 'Acceptance Test Technician and is certified by an authorized 'Acceptance Test Technician Certification Provider.

'Lighting Controls Acceptance Test eMPLOYER’ is a person or entity who is the employer of a 'Lighting Controls 'Acceptance Test Technician and certified by an authorized 'Lighting Controls 'Acceptance Test Technician Certification Provider.

'Mechanical 'Acceptance Test EMPLOYER is a person or entity who is the employer of a 'Mechanical 'Acceptance Test Technician and certified by an authorized 'Mechanical 'Acceptance Test Technician Certification Provider.

'Acceptance Test TeCHNICIAN Certification Provider is an agency, organization or entity approved by the Energy Commission to train and certify 'Acceptance Test Technicians and 'Acceptance Test Employers according to the requirements of Sections 10-103.1or 2.

'Lighting Controls 'Acceptance Test TECHNICIAN Certification Provider is an agency, organization or entity approved by the Energy Commission to train and certify 'Lighting Controls 'Acceptance Test Technicians and Lighting Controls 'Acceptance Test Employers according to the requirements of Section 10-103.1.

'Mechanical 'Acceptance Test TECHNICIAN Certification Provider is an agency, organization or entity approved by the Energy Commission to train and certify 'Mechanical 'Acceptance Test Technicians and 'Mechanical 'Acceptance Test Employers according to the requirements of
Section 10-103.2.

'ACM means ALTERNATIVE CALCULATION METHOD are compliance software, or alternative component packages, or exceptional methods approved by the Commission under Section 10-109. ACMs are also referred to as Compliance Software.

'ACM APPROVAL MANUALS are the documents establishing the requirements for Energy Commission approval of Compliance Software used to demonstrate compliance with the Building Energy Efficiency Standards for Residential and Nonresidential Buildings currently adopted by the Energy Commission.

'ACM REFERENCE ’MANUAL is the document establishing the procedures required to implement Sections 140.1 and 150.1 of Title 24, Part 6 of the California Code of Regulations in Compliance Software.

'ALTERNATIVE COMPONENT PACKAGE is a set of building measures whose aggregate calculated energy use is less than or equal to the maximum allowed Energy Budget.

'APPLIANCE EFFICIENCY REGULATIONS are the regulations in Title 20, Section 1601 et. seq. of the California Code of Regulations.

'APPROVED CALCULATION METHOD is compliance software, or alternative component packages, or exceptional methods approved under Section 10-109.

'BUILDING ENERGY EFFICIENCY STANDARDS are those regulations contained in Title 24, Part 6 of the California Code of Regulations.

'BUILDING PERMIT is an electrical, plumbing, mechanical, building, or other permit or approval, that is issued by an enforcement agency, and that authorizes any construction that is subject to Part 6.

'CALIFORNIA ENERGY COMMISSION is the California State Energy Resources Conservation and Development Commission.

'COMMISSION is the California State Energy Resources Conservation and Development Commission.

'COMPLEX MECHANICAL SYSTEMS are defined here for the purposes of complying with the Design Phase Review component of Section 10-103(a)1. Complex Mechanical Systems are systems that include 1) fan systems each serving multiple thermostatically controlled zones, or 2) built-up air handler systems (non-unitary or non-packaged HVAC equipment), or 3) hydronic or steam heating systems, or 4) hydronic cooling systems. Complex systems are NOT the following: unitary or packaged equipment 'listed in Tables 110.2-A, 110.2-B, 110.2-C, and 110.2-E, that each serve one zone, or two-pipe, heating only systems serving one or more zones.

'COMPLIANCE APPROACH is any one of the allowable methods by which the design and construction of a building may be demonstrated to be in compliance with Part 6. The 'compliance approaches are the performance 'compliance approach and the prescriptive 'compliance approach. The requirements for each 'compliance approach are set forth in Section 100.0(e)2 of Part 6.

'COMPLIANCE DOCUMENT is any of the documents specified in Section 10-103(a) utilized to demonstrate compliance with Part 6 (i.e., Certificate of Compliance, Certificate of Installation, Certificate of Acceptance, and Certificate of Verification).

'COMPLIANCE SOFTWARE is software that has been approved pursuant to Section 10-109 of Part 1.

'CONDITIONED FLOOR AREA is the “'conditioned floor area” as defined in Section 100.1(b) of Part 6.

'CRRC-1 is the Cool Roof Rating Council document titled “Product Rating Program”.

'DATA REGISTRY is a web service with a user interface and database maintained by a Registration Provider that complies with the applicable requirements in Reference Joint Appendix JA7, with guidance from the 'Data Registry Requirements 'Manual, and provides for registration of residential or nonresidential compliance documentation used for demonstrating compliance with Part 6.

'RESIDENTIAL DATA REGISTRY’ is a 'data registry’ that is maintained by a HERS Provider that provides for registration, when required by Part 6 of all residential compliance documentation and the nonresidential Certificate of Verification.

'NONRESIDENTIAL DATA REGISTRY’ is a 'data registry’ that is maintained by a Registration Provider approved by the Commission that provides for registration, when required by Part 6 of all nonresidential compliance documentation. However, nonresidential data registries may not provide for registration of nonresidential Certificates of Verification.

'DATA REGISTRY REQUIREMENTS MANUAL’ is a document that provides additional detailed guidance regarding the functional and technical aspects of the 'data registry requirements given in Joint Appendix JA7.

'DOCUMENTATION AUTHOR is a person who prepares a Title 24 Part 6 compliance document that must subsequently be reviewed and signed by a responsible person in order to certify compliance with Part 6.

'ENERGY BUDGET is the “energy budget” as defined in Section 100.1(b) of Part 6.

'ENERGY COMMISSION is the California State Energy Resources Conservation and Development Commission.

'ENFORCEMENT AGENCY is the city, county, or state agency responsible for issuing a building permit.

'EXCEPTIONAL METHOD is a method for estimating the energy performance of building features that cannot be adequately modeled using existing Compliance Software and that is approved by the Executive Director.

'EXECUTIVE DIRECTOR is the executive director of the Commission.

'FIELD TECHNICIAN is a person who performs acceptance tests in accordance with the specifications in Reference Joint Appendix NA7, and reports the results of the acceptance tests on the Certificate of Acceptance in accordance with the requirements of Section 10-103(a)4.

'HERS is the California Home Energy Rating System as described in Title 20, Chapter 4, Article 8, Section 1670.

'HERS PROVIDER is an organization that administers a home energy rating system as described in Title 20, Chapter 4, Article 8, Section 1670.

'HERS PROVIDER 'DATA REGISTRY is a 'data registry maintained by a 'HERS provider.

'HERS RATER is a person who has been trained, tested, and certified by a 'HERS Provider to perform the field verification and diagnostic testing required for demonstrating compliance with the Part 6 as described in Title 20, Chapter 4, Article 8, Section 1670(i).

'HVAC SYSTEM is the “'HVAC system” as defined in Section 100.1(b) of Part 6.

'MANUFACTURED DEVICE is the “'manufactured device” as defined in Section 100.1(b) of Part 6.

'NFRC 100 is the National Fenestration Rating Council document titled “'NFRC 100: Procedure for Determining Fenestration Product U-factors.” (2011) 'NFRC 100 includes procedures for the Component Modeling Approach (CMA) and site built fenestration formerly included in a separate document, 'NFRC 100-SB.

'NFRC 200 is the National Fenestration Rating Council document titled “'NFRC 200: Procedure for Determining Fenestration Product Solar Heat Gain Coefficients and Visible Transmittance at Normal Incidence.” (2011),

'NFRC 202 is the National Fenestration Rating Council document titled “'NFRC 202: Procedures for Determining Translucent Fenestration Product Visible Transmittance at Normal Incidence.” (2011).

'NFRC 203 is the National Fenestration Rating Council document titled “'NFRC 203: Procedure for Determining Visible Transmittance of Tubular Daylighting Devices.” (2012),

'NFRC 400 is the National Fenestration Rating Council document titled “'NFRC 400: Procedure for Determining Fenestration Product Air Leakage.” (2010).

'PART 6 is Title 24, Part 6 of the California Code of Regulations.

'PUBLIC ADVISER is the Public Adviser of the Commission.

'R-VALUE is the measure of the thermal resistance of insulation or any material or building component expressed in ft²-hr-°F/Btu.

'Record Drawings are drawings that document the as installed location and performance data on all lighting and space conditioning system components, devices, appliances and equipment, including but not limited to wiring sequences, control sequences, duct and pipe distribution system layout and sizes, space conditioning system terminal device layout and air flow rates, hydronic system and flow rates, and connections for the space conditioning system. 'Record drawings are sometimes called “as built.”

'REFERENCE APPENDICES are the support document for the Building Energy Efficiency Standards and the ACM Approval Manuals. The document consists of three sections: the 'Reference Joint Appendices (JA), the 'Reference Residential Appendices (RA), and the 'Reference Nonresidential Appendices (NA) currently adopted by the Energy Commission.

'REFERENCE JOINT APPENDICES are the 'Reference Joint Appendices currently adopted by the Energy Commission.

'REFERENCE NONRESIDENTIAL APPENDICES are the 'Reference Nonresidential Appendices currently adopted by the Energy Commission.

'REFERENCE RESIDENTIAL APPENDICES are the 'Reference Residential Appendices currently adopted by the Energy Commission.

'REGISTERED DOCUMENT is a document that has been submitted to a residential or ‘nonresidential data registry for retention, and the data registry has assigned a unique registration number to the document.

'REGISTRATION PROVIDER is an organization that administers a data registry service that conforms to the requirements in Reference Joint Appendix JA7.

'STANDARD DESIGN BUILDING is a “'Standard Design Building” as defined in Section 100.1(b) of Part 6.

NOTE: Authority: Sections 25402 and 25402.1, and 25213, Public Resources Code. Reference: Sections 25007, 25402 and 25402.1, 25402.4, 25402.5, 25402.8 and 25910, Public Resources Code.