## 10-113 – CERTIFICATION AND LABELING OF ROOFING PRODUCT REFLECTANCE AND EMITTANCE

This section establishes rules for implementing labeling and certification requirements relating to reflectance and emittance for roofing products for showing compliance with Sections 140.1, 140.2, 140.3(a)1, 141.0(b)2B, 150.1(c)11, 150.2(b)1H, and 150.2(b)2 of Title 24, California Code of Regulations, Part 6. This section also provides for designation of the Cool Roof Rating Council (CRRC) as the supervisory entity responsible for administering the state's certification program for roofing products, provided CRRC meets specified criteria.

### (a) Labeling Requirements.

Every roofing product installed in construction to take compliance credit or meet the prescriptive requirements for reflectance and emittance under Sections 140.1, 140.2, 140.3(a)1, 141.0(b)2B, 150.1(c)11, 150.2(b)1H or 150.2(b)2 shall have a clearly visible packaging label that lists the emittance and the initial and 3-year aged solar reflectance, or a CRRC approved accelerated aged solar reflectance, tested in accordance with CRRC-1.

Packaging for liquid-applied roof coatings shall state the product meets the requirements specified in Section 110.8(i)4.

### (b) Certification Requirements.

Every roofing product installed in construction to take compliance credit or meet the prescriptive requirements for reflectance and emittance under Sections 140.1, 140.2, 140.3(a)1, 141.0(b)2B, 150.1(c)11, 150.2(b)1H or 150.2(b)2 shall be certified by CRRC or another supervisory entity approved by the Commission pursuant to Section 10-113(c).

### (c) Designation of Supervisory Entity.

The CRRC shall be the supervisory entity to administer the certification program relating to reflectance and emittance ratings for roofing products, provided the Commission determines that the CRRC meets the criteria in Section 10-113(d).

1. The Commission may consider designating a supervisory entity other than CRRC if the Commission determines that the CRRC is not meeting the criteria in Section 10-113(d). Such other supervisory entity shall meet the criteria in Section 10-113(d) prior to being designated.

2. The Commission shall periodically review, at least annually, the structure and operations of the supervisory entity to ensure continuing compliance with the criteria in Section 10-113(d). The supervisory entity shall provide an annual report to the Commission explaining all of the measures it has taken to comply with the criteria in Section 10-113(d).

### (d) Criteria for Supervisory Entity.

1. Membership in the entity shall be open on a nondiscriminatory basis to any person or organization that has an interest in uniform performance ratings for roofing products, including, but not limited to, members of the roofing industry, building industry, design professionals, specifiers, utilities, government agencies, and public interest organizations. The membership shall be composed of a broad cross section of those interested in uniform thermal performance ratings for roofing products.

2. The governing body of the entity shall reflect a reasonable cross-section of the interests represented by the membership.

3. The entity shall maintain a program of oversight of product manufacturers, laboratories, and independent certifying organizations that ensures uniform application of the CRRC testing and rating procedures, labeling and certification, and such other rating procedures for other factors that improves the accuracy of properties of roofing products affecting energy performance as the CRRC and the Commission may adopt.

4. The entity shall require manufacturers and independent certifying organizations within its program to use only laboratories accredited by the supervisory entity to perform tests under the CRRC rating procedure.

5. The entity shall maintain appropriate guidelines for testing laboratories and manufacturers, including requirements for adequate:

A. Possession and calibration of equipment;

B. Education, competence, and training of personnel;

C. Quality control;

D. Record keeping and reporting;

E. Periodic review (including but not limited to, blind testing by laboratories; inspections of products; inspections of laboratories, and manufacturing facilities);

F. Challenges to certified ratings; and

G. Guidelines to maintain the integrity of the program, including, but not limited to, provisions to avoid conflicts of interest within the rating and certification process’.

6. The entity shall be a nonprofit organization and shall maintain reasonable, nondiscriminatory fee schedules for the services it provides, and shall make its fee schedules, the financial information on which fees are based, and financial statements available to its members for inspection.

7. The entity shall provide hearing processes that give laboratories, manufacturers and certifying agencies a fair review of decisions that adversely affect them.

8. The entity shall maintain a certification policy committee, whose procedures are designed to avoid conflicts of interest in deciding appeals, resolving disputes and setting policy for the certifying organizations in its program.

9. The entity shall publish at least annually a directory of products certified and decertified within its program.

10. The entity itself shall be free from conflict-of-interest ties or to undue influence from any particular roofing product manufacturing interest(s), testing or independent certifying organization(s).

11. The entity shall provide or authorize the use of labels that can be used to meet the requirements for showing compliance with the requirements of Sections 140.1, 140.2, 140.3(a)1, 141.0(b)2B, 150.1(c)11, 150.2(b)1H and 150.2(b)2, and this section.

12. The entity's certification program shall allow for multiple participants in each aspect of the program to provide for competition between manufacturers and between testing labs.

NOTE: Authority: Section 25402.1, Public Resources Code. Reference: Section 25402.1, Public Resources Code.

### (a) Certification Requirements for Manufactured Equipment, Products, and Devices.

Part 6 limits the installation of manufactured equipment, products, and devices to those that have been certified as specified by Sections 110.0 and 110.1.

#### TABLE 100.0-A APPLICATION OF STANDARDS

Occupancies | Application | Mandatory | Prescriptive | Performance | Additions/Alterations
General Provisions for All Buildings | 100.0, 100.1, 100.2, 110.0,
Nonresidential, High-Rise Residential, And Hotels/Motels | General | 120.0 | 140.0, 140.2 | 140.0, 140.1 | 141.0
Envelope (conditioned) | 110.6, 110.7, 110.8, 120.7 | 140.3
Envelope (unconditioned process spaces) | N.A. | 140.3(c)
HVAC (conditioned) | 110.2, 110.5, 120.1, 120.2, 120.3, 120.4, 120.5, 120.8 | 140.4
Water Heating | 110.3, 120.3, 120.8, 120.9 | 140.5
Indoor Lighting (conditioned, process spaces) | 110.9, 120.8, 130.0, 130.1, 130.4 | 140.3(c), 140.6
Indoor Lighting (unconditioned and parking garages) | 110.9, 120.8, 130.0, 130.1, 130.4 | 140.3(c), 140.6 | N.A.
Outdoor Lighting | 110.9, 130.0, 130.2, 130.4 | 140.7
Electrical Power Distribution | 110.11, 130.5 | N.A.
Pool and Spa Systems | 110.4, 110.5 150.0(p) | N. A. | 141.0
Solar Ready Buildings | 110.10 | N.A. | 141.0(a)
Covered Processes1 | Envelope, Ventilation, Process Loads | 110.2, 120.6 | 140.9 | 140.1 | 120.6, 140.9
Signs | Indoor and Outdoor | 130.0, 130.3 | 140.8 | N.A. | 141.0, 141.0(b)2H
Low-Rise Residential | General | 150.0 | 150.1 (a, c) | 150.1 (a, b) | 150.2(a), 150.2(b)
Envelope (conditioned) | 110.6, 110.7, 110.8, 150.0, 150.0(a), 150.0(b), 150.0(c), 150.0(d), 150.0(e), 150.0(g)
HVAC (conditioned) | 110.2, 110.5, 150.0(h), 150.0(i), 150.0(j), 150.0(m), 150.0(o)
Water Heating | 110.3, 150.0(j, n)
Indoor Lighting (conditioned, unconditioned and parking garages) | 110.9, 130.0, 150.0(k)
Outdoor Lighting | 110.9, 130.0, 150.0(k)
Pool and Spa Systems | 110.4, 150.0(p) | N. A. | N.A. | 150.2(a), 150.2(b)
Solar Ready Buildings | 110.10 | N. A. | N.A. | N.A.
1 Nonresidential, high-rise and hotel/motel buildings that contain covered processes may conform to the applicable requirements of both occupancy types 'listed in this table.